From lori!cmcl2!yale!cs.utexas.edu!uunet!ibmpa!dolphin.tcspa.ibm.com!mlewis Wed Mar 14 10:36:10 EST 1990
Article 2273 of comp.sys.ibm.pc.rt:
Path: lori!cmcl2!yale!cs.utexas.edu!uunet!ibmpa!dolphin.tcspa.ibm.com!mlewis
>From: mlewis@dolphin.tcspa.ibm.com (Mark S. Lewis)
Newsgroups: comp.sys.ibm.pc.rt
Subject: IBM 8514 source code (part 1 of 6) for X11 Release 4
Keywords: V1.32_kit.1 8514 X11R4
Message-ID: <4471@ibmpa.UUCP>
Date: 12 Mar 90 23:15:11 GMT
Sender: news@ibmpa.UUCP
Reply-To: mlewis@ibmsupt.UUCP
Followup-To: comp.sys.ibm.pc.rt
Organization: IBM AWD, Palo Alto
Lines: 1650

Subject: IBM 8514 source code (part 1 of 6) for X11 Release 4
Index: ../mit/server/ddx/ibm/ibm8514

Description:	
IBM has decided to provide X11 source code for the 8514 display
adapter.  This is the same code used to build the object files
included in the X11 Release 4 distribution.  This code supports
servers for both AIX and IBM/4.3 on their respective platforms.

	V1.32_kit.1	59,103 Bytes
	V1.32_kit.2	61,796 Bytes
	V1.32_kit.3	60,982 Bytes
	V1.32_kit.4	62,729 Bytes
	V1.32_kit.5	54,871 Bytes
	V1.32_kit.6	29,170 Bytes

Installation:	
This code is provided in a 6-part shell archive.  Before you
install it, you should save your current code.  You should save
the Imakefile in the ibm server directory.  You also should save
the entire ibm8514 directory by moving and remaking it.

	cd ../mit/server/ddx/ibm
	cp Imakefile Imakefile.orig
	mv ibm8514 ibm8514.orig
	mkdir ibm8514
	
Next, edit this header from each part, and feed the rest to
/bin/sh.  Proceed to make the server as instructed in the
X11 release notes.

	sh < V1.32_kit.1

---- 1620 lines deleted to save space, since we don't care about the 8514 ----
