
       Release 3.22 ISO.EXE fixes the problem with application
       writes from Expanded Memory, and the Wang WP / Samna /
       AS/Gateway SBS MLU low memory/stack corruption problem.

         1.  To install the new ISO.EXE, put the floppy in the A:
             drive and type A:UPDATE.

         2.  If the B: drive must be used, then when UPDATE comes
             back with the floppy error ("Abort, Retry, Ignore?" or
             "Abort, Retry, Fail?")  "Ignore" or "Fail" the
             command.  UPDATE will then look for ISO.EXE on the B:
             drive.

         3.  The installation can be checked by running NETSTAT on
             the local machine and checking that the software
             version number is 3.22.

         4.  If for some reason the update doesn't work, save the
             current ISO.EXE to OLDISO.EXE in the ATTNET directory
             and copy over ISO.EXE from the install floppy to the
             ATTNET directory.
