LSR OD 8 Single Register Block Print (program par.)
0r,ta15r	ta30r	ao30r	td17r	ao30r	td12r	ao30r	td19r	ao30r
td36r	10r,ao30r	si126	cs	ad1	ts3t	ca	td22r
ca	td23r	cs	20r,ad1	ts4t	ca	sp	ao22r	ao3t
cp31r	ca53r	rc0	si92	30r,sp	ao4t	cp36r	ca53r	rc0
sp19r	cs	ad50r	cp47r	su50r	40r,ts2t	ao2t	cp44r	sp22r
ca52r	rc0	sp41r	ca51r	rc0	sp22r	50r,+5	1.13000	0.21000
1.23000
END OF SUBROUTINE
{61}m