fc TAPE 1244 m25 ANELEX CONVERSION FOR PROGRAM PRINT PROGRAM
OCTAL	DA1.12540|
50|a3,cav2
cf200
spa4
a4,tsv2	|store flexocode
srh12
adc2
a1,cf400
spf40	| t
spa3	|not used
spf42	|z
spf43	|back space
spf44	|l
spf45	|tab
spf46	|w
spa3		|not used
spf50	|h
spf51	|carriage return
spf52	|y
spa3		|not used
spf54	|p
spa3		|not used
spf56	|q
spa3		|not used
spf60	|o
spf61	|stop
spf62	|b
spa3		|not used
spf64	|g
spa3		|not used
spf66	|9
spa3		|not used
spf70	|m
spf71	|upper case
spf72	|x
spa3		|not used
spf74	|v
spf75	|lower case
spf76	|0
spa3		|nullify and not used
spa3		|not used
spf2	|e
spf3	|8
spa3		|not used
spf5	|1_
spf6	|a
spf7	|3
spf10	|space
spf11	|=
spf12	|s
spf13	|4
spf14	|i
spf15	|+/
spf16	|u
spf17	|2
spa3		|color change,not used
spf21	|.)
spf22	|d
spf23	|5
spf24	|r
spf25	|1
spf26	|j
spf27	|7
spf30	|n
spf31	|,(
spf32	|f
spf33	|6
spf34	|c
spf35	|--
spf36	|k
spa3		|not used
v2,si0	|flexocode
1v2,si0	|case control
c2,si40a1	|start of flexo table
c3,si1	|column counter
1c3,0.06315
2c3,+10
3c3,+120
4c3,+76
5c3,1.70010	|go to top of page
6c3,1.70400	|single space
7c3,si701
f40,ca43a2	|set up t

spp1
f42,ca51a2	|set up z
spp1
f43,cac3	|accomplish back space
su1
tsc3
cp0	|back space off page
sp1f10
f44,ca33a2	|set up l
spp1
f45,cac3	|set up tab
mh1c3
ad1
mh2c3
slh17
tsc3
su3c3
cpf10
b2,ca4c3
tsc3	|reset column counter
ca5f49
b1,tsf58
ca1
ts1f58
ca7c3
si244	|printer activate
bo1y1
ca7c3
si17
bi1y1
ca6c3
ts700y1	|clear printer image
spa3
f46,ca46a2	|set up w
spp1
+0
f50,ca27a2	|set up h
spp1
f51,ca6c3	|set up carriage return
ts2f46
caf58
ad70a2
td6r
ca2f46
ts0
ca1
tsc3
caf49
spb1
f52,ca50a2	|set up y
spp1
f54,ca37a2	|set up p
spp1
f56,ca40a2	|set up q
spp1
f61,ca5c3	|set up stop
sp1f51
f62,ca21a2	|set up b
spp1
f64,ca26a2	|set up g
spp1
f66,ca1v2	|set up 9
cp4r
ca63a2
spp1
ca17a2
spp1
f70,ca34a2	|set up m
spp1
f71,cs0
ts1v2	|set case control to upper case
spa3
f72,ca47a2	|set up x
spp1
f74,ca45a2	|set up v
spp1
f75,ca0	|set case control to lower case
ts1v2
spa3
f76,ca1v2	|set up 0
cp4r
f60,ca52a2	|lower case letter or no.
spp1
ca6a2	|exp. zero
spp1
f2,ca24a2	|set up e
spp1
f3,ca1v2	|set up 8
cp4r
ca62a2
spp1
ca16a2
spp1
f5,ca1v2	|set up|_
cpf10
ca1a2
spp1
f6,ca20a2	|set up a
spp1
f7,ca1v2	|set up 3
cp4r
ca55a2
spp1
ca11a2
spp1
f10,aoc3	|set up space bar
dm17a2
cpf8
dm17a2
cpf18
dm17a2
cpf19
dm17a2
cpf28
dm17a2
cpf29
dm17a2
cpf38
dm17a2
cpf39
dm17a2
cpf48
spb2
f8,md0
adf49
f9,tsf58
clc20
ts1f58
spa3
f18,md0
ad1f49
spf9
f19,md0
ad2f49
spf9
f28,md0
ad3f49
spf9
f29,md0
ad4f49
spf9
f38,md0
ad5f49
spf9
f39,md0
ad6f49
spf9
f48,md0
ad7f49
spf9
f49,y1
70y1
160y1
250y1
340y1
430y1
520y1
610y1
f58,y1	|specifies  address of first register in group
+1	|column within group
srh1
f11,ca2a2	|set up =
adf58
td10r
ca1f58
ad2f58
ts7r
ca1
srh0
ab0
ca66a2
spp1
f12,ca42a2	|set up s
spp1
f13,ca1v2	|set up 4
cp4r
ca56a2
spp1
ca12a2
spp1
f25,ca1v2	
cp4r
f14,ca53a2	|set up I and 1
spp1
ca7a2	|exp.1
spp1
f15,ca1v2	|set up +/
cp4r
ca4a2
spp1
ca1a2
spp1
f16,ca44a2	|set up u
spp1
f17,ca1v2	|set up 2
cp4r
ca54a2
spp1
ca10a2
spp1
f21,ca1v2	|set up .)
cp4r
ca3a2
spp1
ca65a2
spp1
f22,ca23a2	|set up d
spp1
f23,ca1v2	|set up 5
cp4r
ca57a2
spp1
ca13a2
spp1
f24,ca41a2	|set up r
spp1
f26,ca31a2	|set up j
spp1
f27,ca1v2	|set up 7
cp4r
ca61a2
spp1
ca15a2
spp1
f30,ca35a2	|set up n
spp1
f31,ca1v2	|set up ,(
cp4r
ca5a2
spp1
ca64a2
spp1
f32,ca25a2	|set up f
spp1
f33,ca1v2	|set up 6
cp4r
ca60a2
spp1
ca14a2
spp1
f34,ca22a2	|set up c
spp1
f35,ca1v2	|set up --
cp4r
ca2a2
spp1
ca66a2
spp1
f36,ca32a2	|set up k
p1,adf58	|print routine
td7r
ca1f58
ad2f58
ts6r
ca1
srh0
ab0
spf10
a2,+0
+1
+2
+3
+4
+5
+6
+7
si10
si11
si12
si13
si14
si15
si16
si17
si20
si21
si22
si23
si24
si25
si26
si27
si30
si31
si32
si33
si34
si35
si36
si37
si40
si41
si42
si43
si44
si45
si46
si47
si50
si51
si52
si53
si54
si55
si56
si57
si60
si61
si62
si63
si64
si65
si66
si67
si70
DITTO
710|y1,
START AT 0
