LSR MA7 LEAST SQUARE MATRIX
MULITIPLE
zt1={61}
0r,ta153r	ta13r	ao153r	td28r	ao153r	td31r	ao153r	td33r	ao153r
td11r	ao153r	11r,ca	ts12t	13r,ca	ts4t	slh1	ts11t	ad170r
ts7t	mh7t	slh14	ad12t	ts6t	cs6t	ad12t	srh1	su4t
ts5t	28r,cs	ad1	ts8t	31r,ca	ts9t	33r,ca	ts10t	ca12t
td40r	IN	ica168r	39r,IN	40r,its	OUT	ao40r	ao40r	ao5t
cp39r	sp50r	47r,ca75r	su171r	cp66r	50r,ca9t	ad172r	ex9t
si451	ca172r	55r,bi13t	ca10t	ad172r	ex10t	si451	ca172r
61r,bi13t+zt1+zt1	ca55r	td75r	ca61r	td87r	66r,ca6t	td88r
td89r	69r,ca12t	td84r	td85r	cs4t	ts5t	74r,IN	75r,ica	itst
||||||||||
ica173r	its2t	isp84r	80r,IN	icat	imr2t	its2t	84r,iad	85r,its
ica2t	87r,imr	88r,iad	89r,its	OUT	ca170r	dm0	ab84r	td85r
ab88r	td89r	ao5t	cp80r	cs4t	ts5t	ca84r	su170r	sp112r
104r,IN	icat	imr2t	its2t	108r,iad	109r,its	OUT	ca108r	112r,ad7t
td108r	td109r	ao5t	cp104r	ca170r	dm0	ab87r	ab75r	ao8t
cp47r	ca170r	tst	ad12t	td139r	ad11t	td141r	cs4t	ad1
ts5t	ca0	ts1t	134r,ca1t	su167r	ex1t	ts2t	138r,IN
139r,ica	140r,IN	141r,its	OUT	ca141r	ad11t	td141r	ao2t
cp140r	ao5t	cp161r	cs167r	ts167r	cp154r	153r,sp	154r,ca7t
tst	cs4t	ad170r	ts5t	ao1t	ao1t	161r,ca139r	adt
td139r	ad11t	td141r	sp134r	167r,+1	168r,+.0	170r,+2	171r,ica12t+zt1+zt1
172r,zt1+zt1	173r,+1.0
END OF SUBROUTINE
||||||||||
{61}m