fc TAPE 126-50-1608 ROSS MIV GROUP ZERO
(24,6)	DECIMAL
|Preset Parameter Assignments
pp1=0.30000	pp2=+20	pp3=+9	pp4=+24	pp5=+24	pp6=+4	pp7=+24	pp8=+4	pp9=+2	pp10=0
pp11=+6	pp12=+6	pp13=+12	pp14=0.04001	pp15=pp14+1408	pp16=pp15+1408	pp17=pp16+1153
pp18=pp17+300	pp19=pp18+1409	pp20=pp19+321	pp21=pp20+1220	pp22=pp21+0	pp23=pp22+540
pp24=pp23+540	pp25=pp14+2	pp26=pp15+5	pp27=pp16+20	pp28=pp17+5	pp29=pp18+10
pp30=pp19+10	pp31=pp20+20	pp32=0
|Set Call Address Listings
DApp14+1|0.04000+2s1+1	0.14000+16x4+1	DApp16+10|b3+1	DApp16+12|5q6+1	DApp17+2|2d19+1
|Set Section Address Listings
DApp25+1|3s1	a8	DApp27+9|p7
|Main Evaluation Program
DA32|32|sps1	sp32	capp25-pp14+35	0.04000+2s1+1	0.14000+16x4+1	3s1	a8	DApp14|capp25-pp14+35
|0-0 Pre-Loop Setup
DApp14+5|39|r13,sp1a13	IN	isc1	icr4	isc2	icr3	isc4	isc3	icr9
icah2	idvh7	idvk8	its26b1	icap11	isp1z3	itsb1
icap11	ispz3	its4b1	ics4b1	its4b1	ica2p11	imr4b1	itsb2	ics2p11	imrb1	its4b2
icam2	its2b2	its2b1	sps1
|0-1 Check Initial Conditions Data
p7,ca2i1	td2r6	ca1a14	tsv10	ca3a14	tsd4	ca5a14	tss14	ca7a14	tsq3
ca9a14	td3d5	ca0	tsn8	cac2	su2a3	cpy1	mha3	slr14
ts1709	su3a3	cpy2	y1,cac2	ts2a3	mha3	slr15	adf2	0.01703	ca1a3	bia1
cac2	mhu4	slr15	adi5	0.01703	ca4a3	bia4	ca0	ts1709
|0-2 Launching Velocity
y2,IN	isc0	icab2	iada1+c	itsu6	imru6	its20b1	ica2b2	iad2a1+c	its2u6	imr2u6
iad20b1	its20b1	ica4b2	iad4a1+c	its4u6	imr4u6	iad20b1	spz2	its6u6
|0-3 Yaw Angle Correction
icaa1+c	imru6	itsv2	ica2a1+c	imr2u6	iadv2	itsv2	ica4a1+c	imr4u6	iadv2	itsv2
idvh4	idv6u6	isp6z4	its2v2	d6,ica6u6	idvk8	its20b1	OUT	cag10
sps5	itsa10	imr2i7	idv20b1	iexa10	imrk7	imr2v2	imr2v2	its22b1
|0-4 Windage Jump Correction
ica2b2	imr4u6	its12b1	ics4b2	imr2u6	iad12b1	its12b1	imr12b1	its18b1	icsb2	imr4u6
its14b1	ica4b2	imru6	iad14b1	its14b1	imr14b1	iad18b1	its18b1	icab2	imr2u6	its16b1
ics2b2	imru6	iad16b1	its16b1	imr16b1	iad18b1	spz2	its4v2	ica2v2	idv4v2	imrj4
its18b1	ica12b1	imr18b1	iadu6	its6b1	imr6b1	iex14b1	imr18b1	iad2u6	its8b1	imr8b1
iad14b1	iex16b1	imr18b1	iad4u6	its10b1	imr10b1	iad16b1	spz2	its18b1	ica6b1	idv18b1
itsu7	ica8b1	idv18b1	its2u7	ica10b1	idv18b1	its4u7
||||||||||
|0-5 Yaw Correction
icah4	idv6u6	its12b1	imr12b1	imrh1	idvh7	isu2i7	its18b1	isu2i7	imrh2	imrh3
iada10	iex18b1	imr22b1	idv18b1	iad20b1	d1,its18b1	isuw6	itsw7	icpn7	icsw7
n7,iad2w6	icpn9
|0-6 Linearization for Uo1/a
icaw7	imr2w8	iad2w9	itsa10	icaw7	imr4w8	iad4w9	itsa11	icaw7
imrw8	iadw9	its18b1	icaw7	imr8w8	iad6w9	itsa12	ica2c2	q1,isuw1	itsw2	icpn1
icsw2	n1,iad2w1	icpn3
|0-8 Linearization for u/a
icaw2	imrk6	iadq7	itsq15	icaw2	imr2w3	iad2w4	OUT	ca2w2	tsd3	ts5d3
n2,IN	isua10	imr26b1	its8c2	OUT	ca17c2	0.01703	caa3	bim1	IN	isc2
icac6+c	imr8c2	iadm1+c	its6c6+c
|0-11 Projectile Velocity
d7,ica2c2	imrk8	its2a2	imru7	iexq15	isua12	imr2c2	imr26b1	itsa2	imrb1	iadq15
its6b1	imr6b1	itsq15	ica2a2	imr2u7	its8b1	imr8b1	iadq15	iexa2	imr4b1	iex2a2
imr4u7	iad2a2	its10b1	imr10b1	iada2	spz2	itsq15
|0-12 Projectile Position
d3,ispn5	imrw3	iadw4	isu18b1	its24b1	ispn6	imr4w3	iad4w4	isua11	its20b1	ics24b1
imra12	iad20b1	imr26b1	imr26b1	its20b1	imrb1	iex24b1	imr26b1	imrk8	its22b1	imru7
iad24b1	itsa2
|0-13 Miss Vector and Distance
isu6c6	itsm1	imr6b1	its24b1	ica22b1	imr2u7	its2a2	isu8c6	its8c6	imr8b1
iad24b1	its24b1	ica22b1	imr4u7	iex20b1	imr4b1	iad20b1	its4a2	isu10c6	its4m1
imr10b1	iad24b1	idvq15	its6a2	r6,its4c2	icpq8	isui1
|0-14 Check Iterations
q6,its22b1	OUT	aon8	suw5	cpd18	spp2	d18,0.00335	rd
cps1
|0-15 Check Criterion
IN	ica22b1	d2,icps12
|0-16 Continue Iteration, Find New u/a
isc0	icaa4+c	isua2	imr6b1	its22b1	ica2a4+c	isu2a2	imr8b1	iad22b1	its22b1	ics4a4+c
iad4a2	imr10b1	isu22b1	idvq15	isu6a2	idv8c2	isuq15	iex6a2	idv6a2	iad8c2	idv26b1
iada10	OUT	cat5	sps5	its2c2	s15,ispq1
|0-7 Plynomials for Uo1/a
n9,ica18b1	itsw6	OUT	cag10	sps5	itsw8	icsk4	idvw8	itsw8	idv18b1
its2w8	idv18b1	imrw11	its8w8	ica18b1	OUT	caq12	sps5	its6w9	itsa12	imrw8
its4w8	ica18b1	OUT	cat10	sps5	its2w9	itsa10	ica18b1	OUT	cap10	sps5
itsw9	iex18b1	OUT	caq10	sps5	its4w9	itsa11	isp-1q1
|0-9 Polynomials for u/a
n3,ica2c2	itsw1	OUT	ca3w2	tsd3	ca4w2	ts5d3	cag10	sps5	itsw3	icsk4
idvw3	itsw3	idv2c2	its2w3	idvw1	imrw11	itsk6	ica2c2	OUT	caq12	sps5
itsq7	itsq15	imrw3	its4w3	ica2c2	OUT	cat10	sps5	its2w4	isp1n2
|0-17 Range
s12,icaa2	imra2	itsr3	ica2a2	imr2a2	iadr3	itsr3	ica4a2	imr4a2	iadr3	spz2
its6c2	its2r3	v10,spr11
|0-18 Gun-Aiming Criterion, Z
icau6+c	idv6u6	its12b1+c	ict1v10	imr4m1	its20b1	ica12b1	imrm1	iad20b1	its20b1	ics14b1
imr2m1	isu20b1	its20b1	imr12b1	iadm1	idv6c2	its6b1	imr6b1	its22b1	ica20b1	imr14b1
iad2m1	idv6c2	its8b1	imr8b1	iad22b1	iex20b1	imr16b1	iad4m1	idv6c2	its10b1	imr10b1
iad20b1	spz2	its4c2	isu10a3
|Check Z iterations
its20b1	OUT	ao1n8	suw5	cpv3	sp5q6	v3,0.00335	rd	cps1
|Check Z Criterion
IN	ica20b1	icps13	v4,spv5	ca0	tsn8
|New Firing Conditions
IN	ica6b1	imrb2	its20b1	ica8b1
imr2b2	iad20b1	its20b1	ica10b1	imr4b2	iad20b1
imr6u6	idv4v2	its22b1	imr6u6	its20b1	imr6u6	idvv2	isu22b1	iad2v2
iex2v2	imr20b1	iex6u6	isu6u6	its6u6	imr6u6	its22b1	ics6b1	iad12b1	imr6u6	itsu6	imrb2
itsv2	ics8b1	iad14b1
imr6u6	its2u6	imr2b2	iadv2	itsv2	ics10b1	iad16b1	imr6u6	its4u6	imr4b2
iadv2	iex22b1	isu22b1	itsv2	ispd6
|0-19 Store Target Results
r11,can3	td2r11	ca2c2	tsa6	ao3r11	ao2r11	su7a3	cp2r11	ca3r11	ad5a3	ts3r11
IN
|0-20 Find Error Components
d10,ica2c2	iexe3	its2c2	ica2a2	imrm1	its18b1	icsa2	imr2m1	iad18b1	its18b1	d4,ispd5
imrh4	its2r3	icaa2	imra2	itsr3	ica2a2	imr2a2	iadr3	itsr3	d5,icar3	spz2	iex18b1
idv18b1	its14c2	icaa2	imr4a2	imrm1	its24b1	ica2a2	imr4a2	imr2m1	iad24b1
its24b1	icar3	imr4m1	isu24b1	idv18b1	idv2r3	its16c2
|0-21 Target Error Components
s14,idv2r3	its12c2	ica14c2	idv2r3	its10c2	OUT	d19,0.00331	rd	cpp1
IN	ica14c2	spd16	ts19d16	IN	ica16c2	spd16	0.00655	ca19d16	rc	ca0
0.01655	ca0	rc17d16	rc20d16	rc21d16	rc22d16	sps1
|Set Z loop
ca0	ts1n8	caa14	tdv4	ca2a14	tsv10	ca8a14	tsq3	IN	ispv10
|Set for Gun Iteration
v5,tav4	ca5i1	td2r6	ca4a14	tsd4	ca6a14	tss14	ca10a14	td3d5	sp1v4
|0-23 Store Gun Results
r12,cas8	tde1	e1,ca8c2	ts8a6	ao1e1	aoe1	su8a3	cpe1	ca4c2	sp8e1	ta12e1
ts18a6	ao9e1	ca5c2	sp	ca1e1	ad6a3	ts1e1	ad15a3	td9e1	cac2	ts1c2	e4,sp1r1
ao1a7	dm12a3
cpd8	spa8	d8,sps1	IN	icat1	iadk4	itst1	OUT	aoc2
suc1	cpp7	b3,spp2
|0-24 Set for Gun Errors
s13,isc0	icsu6	iadb2	itsa2	iada1+c	itsm1	ics2u6	iad2b2	its2a2	iad2a1+c	its2m1
ics4u6	iad4b2	its4a2	iad4a1+c	its4m1	ispd10
|0-25 Polynomials for u/a
n5,ica2c2	OUT	cap10	sps5	itsw4	isp3d3	n6,ica2c2	OUT	caq10	sps5
its4w4	isp8d3
q8,ics6a2	isp2r6
|0-26 DOB Subroutine
a8,taa13	caa7	mh13a3	slr15	ad14a3	0.01707	ca1a7	mh13a3	slr15	a9,boa6
ca0	ts1a7	r1,sp5r1	tae4	cac2	tsa7	sp1e4
tae4	caa9	td3r11	ad16a3	td1e1	ad6a3	td9e1	a13,sp	taa13	spr1
|0-27 Scope Coordinates
d16,ta11d16	cs2042	cp6d16	cm2042	ad18d16	sp8d16	ad18d16	cp12d16	td10d16	ca2043
srr0	sp	dm0	cp15d16	sp11d16	ca2043	sp11d16	0.76000	+6	+0	0.00174
1.00000	0.00200
|0-28 Polynomial Subroutine
s5,ta17r	td6r	ad1	td12r
ad18r	td14r	ca0	td11r	IN	its6a2	icxj3	icr	ica	imr6a2	iad+c
ictl3r	icxj3	isp	+2
|0-29 Sine-Cosine Subroutine
z3,iad46r	ita32r	imr40r	its12b1	icp6r	ics12b1	iad42r	icp6r	isu44r	icp33r	isu44r
icp17r	isu44r	icp35r	isu44r	its14b1	ics14b1	its14b1	ica12b1	icp37r	ica14b1	imr14b1
its12b1	imr48r	iad50r	imr12b1	iad52r	imr12b1	iad54r	imr12b1	iad56r	imr14b1	isp
iad44r	isp15r	iad44r	isp17r	ics14b1	its14b1	isp21r	+.636619772	+4.	+1.
+1.570796327	+.00015148419	-.00467376557	+.07968967928	-.64596371106	+1.57079631847
||||||||||
|0-30 Arcsine-Arccosine Subroutine
z4,ita5r	isp6r	its12b1	ics12b1	iad46z3	isp	ita25r	its12b1	icp45r	its16b1	ica44z3
isu16b1	spz2	its14b1	icxj3	icr7	ica29r	imr16b1	iad31r+c	ict17r	imr14b1
iex12b1	icp26r	ica12b1	icxj3	isp	ics12b1	iadk1	isp24r	-.0012624911	+.0066700901
-.0170881256	+.0308918810	-.0501743046	+.0889789874	-.2145988016	+1.5707963050
ics12b1	isp9r
|0-31 Square Root Subroutine
z2,ta2019	ca2043	dm0	cp34r	ab0	cp	mr44r	ad45r	mr2043	ad46r	ts2037
ts1835	cm2042	clc15	cp35r	ca2042	srr1	ts2036	ts1821	ca49r	ts2018	ca2044
ts24b1	sp1924	ca1821	ts2036	ca1835	ts2037	ca24b1	sp42r	su1	ts2042	ca48r
ts2018	sp2019	ca2037	mr47r	ts2037	ts1835	ca2042	ad1	sp16r	ta2018	sp1969
1.63061	0.70660	0.24036	0.55203	ao2019	sp24r
|0-32 Constants and Storage
a2,+0	DITTO	10r|+.1285714328	a3,pp12	pp4	+1000	pp3	pp5	+12	+10
ca9c2	ca17c2	+0	+.0005	pp8-1	pp2	pp1	+9	+8	a10,+.0	a11,+.0
a12,+.0	a14,v5	spr11	isc2	ispd5
icah4	idv2r3	spr12	0.00333	0.00334	18b1	r3	b1,+0	DITTO	
28r|f2,pp22	f3,+16	f4,-6f1	g10,1g10	+5	-.26360580x10-17	+.29363176x10-13	-.12962703x10-9
+.27300916x10-6	-.22400791x10-3	+.14416338	h1,+1.92	h2,+.367	h3,+.0043286	h4,+2870.
h7,+.4	i1,+2.5	i1	+10.	3i1	i2,+200	i5,pp23	i7,-.166666667	+.5	-.5	+.166666667	j3,+0
+0	j4,+62.635504	k1,+3.1415926535	k2,-2047	k4,+1.	k5,+2.	k6,+.0	k7,-8.2	k8,+.94161763
m1,+0	DITTO	8r|m2,+.0	p10,1p10	+5	-.65911606x10-13	+.81634201x10-9	-.43078770x10-5
+.012630531	-26.996788	+39173.2387	p11,+.13	+440.	q7,+.0	q10,1q10	+5
-.58666128x10-13	+.69185197x10-9	-.33459018x10-5	+.84343688x10-2	-11.403677	+6883.4012
q12,1q12	+5	-.96116495x10-17	+.11290374x10-12	-.54272871x10-9	+.13537084x10-5	-.18049075x10-2
+1.088621892	q15,+.0	r3,+.0	+.0	t5,1t5	+3	-2.88504374	+67.37679583	-692.3300090
+3959.854157	t10,1t10	+5	-.20096037x10-15	+.23946791x10-11	-.11813740x10-7
+.30949600x10-4	-.046246085	+35.6170362	u1,+2	u2,+.0	u3,pp7	u4,pp12	u5,pp6-3
u6,+.0	+.0	+.0	+.0	v2,+.0	+.0	+.0
w1,+.0	+.0	w2,+.0	icaw2	ispn5	ispn6	w3,+.0	DITTO	8r|w4,+.0	DITTO
6r|w5,+4	w6,+.0	+.0	w7,+.0	w8,+.0	DITTO	10r|w9,+.0	DITTO	8r|w10,+0	w11,+32.172
u7,+.0	+.0	+.0	+.0	
|0-33 Input-Outout Blocks
a1,+.0	DITTO	24r|a4,+.0	DITTO	24r|a6,+.0	DITTO
8r|e3,+1853.	e2,
|Invariant Storage Flads
OCTAL
2640|c1,	2641|n8,	2643|a7,	2645|c2,	2667|t1,	2671|s1,	2675|q2,	2702|q5,	2706|q3,	2711|x4,
2733|q4,	2740|s4,	2754|s6,	2760|q14,	2765|q13,	2767|q11,	3001|p1,
3005|p2,	3012|p3,	3153|t2,	3173|c5,	3207|c6,b2,
OCTAL
START AT 0
v