*M*      RTBOOT DUMMY GHOST1 REAL-TIME MODULE
*
         CSECT    1
RTBOOT   EQU      %
         DEF      RTBOOT            MODULE BIAS
***********************************************************************
*P*      NAME:    RTBOOT
*,*
*,*      PURPOSE: PROVIDES A DUMMY MODULE AND ENTRY POINT WHICH COULD
*,*               BE REPLACED BY AN INSTALLATION-WRITTEN MODULE.
*,*
*,*      DESCRIPTION:  MODULE IS LOADED WITH GHOST1 AND CONTAINS A
*,*               SINGLE ENTRY POINT:  RT:REBOOT.
***********************************************************************
*F*      NAME:    RT:REBOOT
*,*
*,*      PURPOSE: PROVIDES A DUMMY ENTRY POINT WHICH COULD BE REPLACED
*,*               BY AN INSTTALLATION-WRITTEN ROUTINE.
*,*
*,*      DESCRIPTION:  (SEE 'D' REPORT)
***********************************************************************
*D*      NAME:    RT:REBOOT
*,*
*,*      REGISTERS:  (ALL ARE AVAILABLE TO USER-WRITTEN ROUTINE EXCEPT
*,*               RETURN MUST BE MADE VIA R11)
*,*
*,*      CALL:    BAL,R11
*,*
*,*      INTERFACE:  (UP TO USER)
*,*
*,*      ENVIRONMENT:  CALLED MAPPED/MASTER; INTERRUPTS ENABLED.
*,*
*,*      INPUT:   (ALL MONITOR DEFS ARE AVAILABLE TO USER-WRITTEN
*,*               ROUTINE).
*,*
*,*      OUTPUT:  (UP TO USER)
*,*
*,*      DESCRIPTION:  THIS ROUTINE IS EXECUTED AS A PART OF THE GHOST1
*,*               LOAD MODULE.  IT IS CALLED FOLLOWING THE
*,*               INITIALIZATION OF THE SWAPPING RAD (SYSMAK) EACH TIME
*,*               THE SYSTEM IS BOOTED (OR REBOOTED FOLLOWING A CRASH).
*,*               THIS ROUTINE SHOULD INTERFACE WITH THE FOLLOWING
*,*               USER-WRITTEN ROUTINES (CONTAINED IN THE RTPFSR MODULE)
*,*                    RT:RCVR
*,*                    RT:PWOFF
*,*                    RT:PWON
***********************************************************************
*
         SYSTEM   SIG7
*
         DEF      RT:REBOOT         DUMMY GHOST1 ENTRY POINT
RT:REBOOT     EQU %
*
         B        *11
         END

