
This set of directories contains miscellanious CM I/O system example
programs.  

	maxvideo:
		A program to use the CM and the DataVault as a VCR,
		using the DataCube MaxVideo framegrabber via the CMFS
		file server running on a system with a VMEIO board.

		Also includes a program to play back the movie on an
		Xwindow display.

	maxvideo-driver:
		The CMFS device-driver for the MaxVideo device, to be
		linked into the CMFS file server.

	tape-driver:
		The CMFS device-driver for tape devices.  This is a
		supported part of the fsserver.

	misc-cm:
		A set of address translation functions for use with
		CM_transpose. 

	misc-serial:
		fast-copy.c: a program which uses fancy
		double-buffering to move data between UNIX and the CM
		file system.
		
	
