




        File Name: README.SHD
        Source   : Disk # 2  P/N: 008004812  Rev. 1.05
        Date     : August 9, 1989

        =================================================================

        This  directory contains Drivers for use  on  AutoShade   release
        1.0/1.1.  The directory should contain the following:

                 o ACAD61B.EXE - 640x400 / 256 colors driver
                 o ACAD62B.EXE - 640x480 / 256 colors driver - requires
                                 512k memory
                 o ACAD63B.EXE - 800x600 / 256 colors driver - requires
                                 512k memory
                 o ACADDRV.EXE - Driver installation program. This
                                 program  is started by the main  program
                                 VDRIVER.EXE.
                 o README.SHD  - This file.

        The setup procedure is as follows:

        1. Install AutoShade on your hard disk.

        2. Run the VDRIVER.EXE and  follow the  instructions given by the
           program.

        3. Run ASHADE.BAT.

        4. The  first  time you use it only, configure AutoShade  to  use
           ADI driver.  See CONFIGURING AUTOSHADE below.


        CONFIGURING AUTOSHADE

        1. Select   option  [1]  for  Autodesk  Device Interface  display
           driver and enter the selected interrupt vector.

        2. Select  option [1] for  Autodesk  Device  Interface  rendering
           display driver and enter selected interrupt vector.

        3. Enter  YES  for the  display and  rendering devices sharing  a
           single screen.

        4. Enter YES for "flip screen" requiring a redraw.

        LOADING THE ADI DRIVERS FOR AUTOSHADE

        The ADI drivers are selected exactly as for AutoCAD. All the
        options are available except options 'd' and '256'. To load the
        ADI drivers, type:

               ACADxxB [i] [-yy]

        where xx is the resolution mode (61, 62 and 63).


                                        
        Disk 2               README.SHD                       Page 2



        For more details about the options [i] and [-yy], see README.ACA.

        The  ADI  drivers provided use interrupt 7A as default.  You  can
        select  different  interrupt if required. You must use  the  same
        interrupt value for the ADI drivers and for the ADI display.

        For a printout of this information, type

              A>COPY README.SHD PRN <enter>















































                                        

