




        File Name:  README.VCA
        Source   :  Disk # 3  P/N: 008004813  Rev. 1.05
        Date     :  August 9, 1989

        ====================================================================

        This directory contains drivers for use on VersaCAD version  5.3.
        Note that the current release supports VersaCAD version 5.3 only.
        The directory should contain the following:

                o VCAD61B.COM - driver for 255 colors modes:
                                640 x 400
                                640 x 480 - requires 512K video RAM
                                800 x 600 - requires 512K video RAM
                o VCAD65B.COM - 1024 x 768 (15 colors) driver - requires
                                512K video RAM
                o VCAD67B.COM - 1024 x 768 (3 colors) driver
                o VCADDRV.EXE - Drivers installation program.  This
                                program is started by the main program
                                VDRIVER.EXE.

                o VCAD-B.CFG   - Configuration file for VersaCAD initial
                                set up.

                o README.VCA   - This file.


        The setup procedure is as follows:

                1/ Install VersaCAD on your hard disk, with EGA  selected
                   for Screen Configuration.

                2/ Run VDRIVER.EXE and follow the instructions given by
                   the program.

                3/ You will be told to do initial setup for VersaCAD in
                   order  to  incorporate the  high  resolution  drivers.
                   Simply follow as instructed.


        For a printout of this information, type

            A>COPY README.VCA PRN <enter>

