




        File Name:  README.SKE
        Source   :  Disk # 2  P/N: 008004812  Rev. 1.05
        Date     :  August 9, 1989

        ====================================================================

        The  ADI drivers provided in this disk do not officially  support
        AutoSketch  ver. 1.04.  However, most users will find  that  they
        work satisfactorily on their systems.

        Due  to  memory allocation limitation in AutoSketch,  the  memory
        usage  indicator at the top right corner of the screen  dose  not
        show  the correct figure. Under some circumstances,  this  figure
        may exceed +100%, which causes unpredictable results including  a
        crash. Do not be concerned if the figure is negative. No solution
        is possible unless a future revision of AutoSketch resolves its
        memory allocation problem.

        If  you wish to use the ADI driver, follow the set up  procedure.
        The high resolution drivers that can be used are:

                o  ACAD54B.EXE  - 800 x 600 (16 COLORS)
                o  ACAD65B.EXE  - 1024 x 768 (16 COLORS)
                o  ACAD67B.EXE  - 1024 x 768 (4 COLORS)

        The setup procedure is as follows:

                1/ Install AutoSketch on your hard disk.

                2/ Run the VDRIVER.EXE and follow the instructions  given
                   by the program.

                3/ Run ASKETCH.BAT.

                4/ Configure the AutoSketch to use ADI driver in the
                   first time only.

        The  first time you use AutoSketch with the ADI driver, you  need
        to  configure AutoSketch for the ADI display. Select  option  [1]
        for  Autodesk Device Interface display driver and enter  selected
        interrupt vector.

        LOADING THE ADI DRIVERS FOR AUTOSKETCH

        The ADI drivers are selected exactly as for AutoCAD. All the
        options are available except options 'd' and '256'. To load the
        ADI drivers, type:

               ACADxxB [i] [-yy]

        where xx is the resolution mode (54, 65 and 67)

        For more details about the options [i] and [-yy], see README.ACA.



                                        
        Disk 2               README.SKE                       Page 2



        The  ADI  drivers provided use interrupt 7A as default.  You  can
        select  different  interrupt if required. You must use  the  same
        interrupt value for the ADI drivers and for the ADI display.

        For a printout of this information, type

                A>COPY README.SKE PRN <enter>

















































                                        

