List of Compatible Devices
Synchronous Burst SRAMs

 The TMS320C6201 supports piplined, single-cycle deselect or double-cycle deselect and
selectable burst mode. Part #'s Include Micron  MT58LC128K32D8 128K x 32 Galvantech
GVT71128G36 128K x 36 (only wire up 32-bits) Samsung KM736V789/L  128K x 36 (only wire up
32-bits) NEC uPD4311632L 32K x 32   
 
 Synchronous DRAMs (SDRAMs)  We recommend the following SDRAMs:  Number of Devices Per CE
Part Number Organization Mbytes per CE Speed Sort of 'C6x (a) 2 TMS626162B 512K x 16 x 2
Banks 4 Mbyte 166, 200 MHz (b) 4 TMS626812B 1M x  8 x 2 Banks 8 Mbyte  166, 200 MHz (c)2 
TMS664164 1M x 16 x 4 Banks 16 Mbyte 166, 200 MHz (d) 2 HM5216165 512K x 16 x 2 Banks 4
Mbyte 166, 200 MHz (e) 4 HM5216805 1M x  8 x 2 Banks 8 Mbyte 166, 200 MHz (f) 2 HM5264165 1M
x 16 x 4 Banks 16 Mbyte 166, 200 MHz (g) 2 KM416S1020C 512K x 16 x 2 Banks 4 Mbyte 166, 200
MHz (h) 4 KM48S2020C 1M x  8 x 2 Banks 8 Mbyte 166, 200 MHz (i) 2 KM416S4030B 1M x 16 x 4
Banks 16 Mbyte 166, 200 MHz Note: SDRAM Data Sheets are constantly changing.  To be certain
of operation, the newest data sheet available should be compared to the 'C6201 datasheet in
order to guarantee operation.  Of the memories listed here, some will give more timing
margin than others. For example, the Texas Instruments memories listed here are available at
125 MHz, and if extra margin is needed on the target system, these memories would be an
option. But since different speed grades are available for each part, it is the users
responsibility to verify that timings are met. 


SOCKETS:

Oztec   
510-782-2654 (phone)  
Part Number: SKT-BGA-352-1.27M-35M-CCBO  
Benefits: Can be removed from board.  Very reliable.  Very low inductance.  
Disadvantages: Several hundred dollars cost:

Aries   
Part Number: 2467-114-23  
Benefits: Sub $100 Cost  
Disadvantages: We experienced some manufacturing problmes with early samples.  CTi Technologies  
Part Number: 861-256-0-0X   
