                  TMS320C3x 1996 DSP Starter Kit User's Guide Errata

Document Revision 2.0
Last modified: 2/6/97

The following errors exist in the TMS320C3x DSP Starter Kit User's Guide
Errata (1996 edition): SPRU163A.
---------------------------------------------------------------------------

  1. Page 2-2, sixth line:
     The Host bullet text should read:
          An IBM PC/AT or 100% compatible PC with hard disk system and a
          1.44 megabyte floppy-disk drive and parallel printer port
          communication link
  2. Page 4-3, Figure 4-1:
        o The bubble on the OR gate next to Q1 latch has a buble on the Q1
          signal should be moved down to the Q0 signal, so as to perform
          /Q0 + Q1 logic.
        o The gray block on the left shoudl be labeled host. The gray block
          on the right should be labeled TMS320C31.
        o The /STROBE signal on the right grey block should be labeled as
          /STRB.
        o The /SRAM signal output is missing from the address decode logic
          of the TICPAL22V10Z-25
  3. Page 4-7,Figure 4-4:
        o The ending address of the RAM block 1 should read 809BFFh.
        o The starting address of the Kernel section should read 809F00h.
          The memory map should start like:
          000000h

                       Reserved for boot loader

          000FFFh

          001000h



                       Boot 1

                           EXTERNAL USER_BOOT





          0FFFFFh

          100000h




                                No Decode

          400000h      Boot 2






          7FFFFFh

          800000h

                       Internal memory Mapped Peripherals
                                ........

          ......

  4. Page 4-19: Figure 4-9:
     The Control Register Bit Field D5 should read:
        + 0 = asynchronous
        + 1 = synchronous
  5. Page 4-29, Load file label:
     The black box next to the Load_File routine heading should read
     load_file.
  6. Page 6-4, Table 6-3:
     The following labels need the plural pins:
        o Timer Signals (2 pin) should read Timer Signals (2 pins)
        o Clock Signals (3 pin) should read Clock Signals (3 pins)
        o The Reserved (5 pin) label should read Emulation (5 pins)
  7. Page 5-5, @ prefix bullet,
     The first sentence should read:
          If you use the @ sign as a prefix, the assembler treats the
          operand as the contents of a 24-bit address, specified by @addr.
          The 8 MSBs of the address are specified by the DP registers; the
          16 LSBs are specified by the instruction word.
  8. Page 6-24, page header:
     The page header should read: .loop/.endloop Assemble Code Block
     Repeatedly.
  9. Page 7-7, Command line bullet:
     The second sentence should read:
          When the command or disassembly windows are active, you can enter
          a command by just typing it.
 10. Page 7-10, Table 7-3:
     Third row should read:
          Delete the character to the left of the cursor Backspace
     Fourth row should read:
          Delete the character to the right of the cursor DEL
 11. Page B-3:
     Oscillator bullet, last sentence should read:
          The 'C31 internal clock value is divided by 2 (half frequency).
 12. Page Index-1:
     Replace BA, BD, and BL command with SB, CB, and DB, respectively.
 13. Page Index-2:
     Delete c or com debugger option 7-3entry.
     Replace constants -> symbols as 5-8 with constants -> symbols as 5-11
     Replace debugger -> options -> c or com 7-3 with debugger -> options
     -> LPT 7-3.
     Replace debugger -> options -> h 7-2 with debugger -> options -> help
     7-2.
 14. Page Index-3:
     Replace h debugger option with HELP debugger option
     Replace Init_Systemm 4-30 with Init_Communications 4-30.
     Delete -l option
     Replace LF_Cmd with Load_File.
 15. Page Index-4:
     Replace software breakpoints -> BA, BD, and BL with SB, CB, and DB,
     respectively.

---------------------------------------------------------------------------
 