

	      **********************************************
	      * 					   *
	      *        TMS340 Graphics Library Port	   *
	      *   to TMS34010 Software Development Board   *
	      * 					   *
	      **********************************************


  This directory contains the OEM-specific TMS340 Graphics Library files
  that have been ported to Texas Instrument's TMS34010 Software
  Development Board (SDB).  The 34010 SDB port currently supports the
  following 4 graphics modes:

     mode #   resolution   # colors   # pages	monitor
     ------   ----------   --------   -------	-------
	0      640x480x4      16	 1	NEC MultiSync (analog)
	1      448x480x4      16	 2	NEC MultiSync (analog)
	2      640x480x4      16	 1	SONY MultiScan (analog)
	3      448x480x4      16	 2	SONY MultiScan (analog)

  All graphics modes drive noninterlaced displays.

  Subdirectory \OEMPRIMS contains the hardware-specific TMS340 Graphics
  Library functions that have been ported to the 34010 SDB.  Subdirectory
  \DEMOS contains a series of demonstration programs that run on the
  34010 SDB.  To view the demos (assuming you have installed the 34010
  SDB on your system), change to the \DEMOS subdirectory and run the
  DEMO.BAT batch file.

  The GSP COFF loader utility GSPL.EXE in the \DEMOS subdirectory has
  been configured for a 34010 SDB located in segment 0xD000 of the PC's
  address map.	This was done to avoid address conflicts with certain VGA
  clones.  If your SDB still resides in segment 0xC000, you will need to
  reconfigure the gspl utility by invoking it with the "-c" command-line
  option.

