# @(#)PC.TXT	3.6.1.1 Copyright(C)1992 Xilinx Inc. 5/4/94 23:55:34
# file: pc.err
# date: 06/28/1990; 07/10/90
# what: Xilinx EPLD port_copy system error messages -user text
# Z. K.
0001: [Internal Error - no pin assignment file specified].
0004:Restoring pinout from a %s device and targeting a %s device.
     Please check that you've selected the correct target device.
0005:Cannot copy pin assignment.
0006:Cannot restore pinout from device '%s' onto device '%s'.
     If you want to restore the pinout using a pin-save file,
     please target a device with the same package type and pin count.
0007: [Internal Error in device type '%s'].
0008:Nameless instance found. Placement is not copied.
0009: [Internal Error - user array in environment].
0010:Out of memory.  Cannot continue.
0011:[Internal error: port '%s' placed more than once].
0012:Port '%s' from the pin-save file is no longer in the design.
0015: [Internal Error - design not loaded].
0016: [Internal Error - chip is not loaded].
0017:No pins copied.
0019: [Internal Error - Schematic is already placed].
0020: [Internal Error - One option: PROCESS,IGNORE,RESTORE or FREEZE allowed].
0021: [Internal Error - No option: PROCESS,IGNORE,FREEZE or RESTORE found].
0022:Can't open output file '%s'.
     Please check you have write permission to this file.
0023:Can't open input file '%s'.
0025: [Internal Error. Cannot find  pin '%s' in component '%s'].
0027:Signal '%s' assigned to invalid pin location '%s'.
0032:Unrecognized syntax in pin-save file %s, at line %03d: '%s'.
0033:Port '%s' is specified more than once in the pin-save file %s.
     You can assign it only once.
0034:Assigned pin '%s' does not exist on the target device.
     Please specify a valid pin name.
0035:Physical pin '%s' occurs more than once in pin-save file %s.
     If you edited the file, please assign only one signal to this pin.
0036:Port '%s'(type %s) cannot be placed on pin '%s'(type %s).
0038:Do NOT attach the Pin-assignment Property to non-port '%s',
     attach it to port components only!
0039:Signal '%s' assigned to pin '%s' in the design file, 
     ignoring assignment to pin '%s' in the .vmf file.
0040:Fast Input signal '%s' assigned to non-fast-input pin '%s'.
0041:Signals '%s' and '%s' both assigned to the same pin '%s'.
#
#          Info messages, like headers, dash-lines, etc.

0500:*
*      P I N    C O P Y I N G    S T A R T 
*
0501:*
*        P I N    C O P Y I N G    E N D 
*
0507:*
*      M A N U A L    P I N    A S S I G N M E N T    S T A R T .
*
0508:*
*      M A N U A L    P I N    A S S I G N M E N T    E N D .
*
0509:*
0510:Processed %d port assignments using a pin-assigner symbol
0512:Pin assignment %s in instance %s is overwritten with %s.
0513:Number of saved pins:  %d
0516:Processed %d port assignments using properties
#
# end of file
#



