# @(#)IM.TXT	3.1 Copyright(C)1992 Xilinx Inc. 5/4/94 23:55:32
# file: im.err
# date: 6/28/90
# what: Xilinx EPLD importer error messages -user file
# Z. K.
#
0001:[Internal Error: chip model is not loaded].
0002:Unable to find and open JEDEC input file.
0003:Invalid JEDEC input filename.
0004:Incorrect fuse count: %lu fuses found.
0005:Too many fuses in JEDEC input file.
0006:[Internal Error: bad parameter passed to a procedure].
0007:Expected fuse number %lu, but instead found fuse number %lu.
0008:Too few fuses in JEDEC input file, End-of-file found. 
0009: Did not find fuse number %lu in JEDEC input file.
0010: [Internal Error: Cannot find a bitmap in database].
0011:The input file is for an unknown device '%s' !
#
# end of file
#
