# @(#)UN.TXT	3.1 Copyright(C)1992 Xilinx Inc. 5/4/94 23:56:00
# file: un.err
# date: 6/29/90
# what: Xilinx EPLD PLD UNASM error messages -user file
# Z.K.
0001:Out of memory. Aborting.
0002:Unable to open the input jedec file.
0003:Aborting.
# 0004:Internal Error: Procedure un_ltoa called with bad radix.
0004: [Internal error: bad radix].
0005:Error found at fuse number %u. Input-file is not a proper JEDEC file.
0006:Device is not supported.
0007:Special function not supported.
0008:[Internal Error: Undefined error].
0009:Expected %d fuses, but input file has %d.\
        Is the correct PLD-type selected?
0010:Fuse location %u is too large for current device.
0011:
0012:
0013:
0014:
0015:
0016:
0017:
0018:
0019:
0020:
0021:
0022:
0023:
0024:
0025:
0026:
#
# end of file
#

