Speicherdump:
=============

R0..7:	00 28 00 00 F0 0D 0A 79
Stack:	                         8C F3 1E D3 1F D6 2D 11
	29 32 10 FC 8C EA 8A CE  00 C4 88 80 C8 0C 80 44
	00 00 00 
20:          00 00 8E 00 ED  25 E9 80 48 8C 00 8C 03
30: 28 AF BE E5 E5 E5 E5 00  08 FA 88 C8 02 CC 41 EC
40: EF 5A DF CC 6F 01 82 8F  00 9C 03 03 03 AE 00 00
50: CB EE C8 FF FF FC 08 00  00 00 03 00 88 CC CC 6B
60: 82 00 00 00 4C 00 88 84  00 00 00 00 02 62 03 10
70: 01 A2 01 A2 00 02 00 00  00 0F 00 6B 11 08 00 03


Kommandos:
==========

C
D: Read and dump current sector (532 bytes)
F: format drive
H
N: do nothing
R: read block into buffer
V: verify drive
W: -
X: -
ctrl-L: restart
BI: 10 hour burnin test
BC: -
F!: ???
MS: -
PS: -
RR: read random block (LBA 00.TH1.TL1)
RZ: rezero drive to track 0
PK: park heads
DR: dump 128 bytes data RAM
CL: display Limit flag status
RZ!: rezero drive to track 1


Annahmen:
=========

03D2
12B6
03E7	Read System Track
03F8	Write System Track
0EED	Read LBA
0EF8	Write LBA

00E4.0	SCSI ID
00E4.1	SCSI ID
00E4.2	SCSI ID
00E4.3
00E4.4	1=Config-Jumper closed
00E4.5	0=Track0 reached

00E5	Port

56	08/0A
57	LBA H
58	LBA M
59	LBA L
5A	01 Blocks to read
5B	00/90


