# Firmware and EEPROM Upgrades

From this page, you can access firmware and EEPROM images for Exabyte products and instructions for performing upgrades.

Firmware enables your Exabyte tape drive, library, autoloader, or connectivity solution to correctly interpret commands from software applications. EEPROM (Electrically Erasable Programmable Read-Only Memory) images are custom settings for certain options, such as whether a tape drive compresses data by default. (Only certain models of tape drives use EEPROM images; libraries do not use EEPROM images.)

> Note: When you click on a file for downloading, your browser may display the file instead of saving it to disk. (This problem may occur for files with the following extensions: .out, .hex, .i, .dos, .drv, .com, .tap.) If necessary, use your browser to save the file to your hard drive. Or, configure a new MIME type in your browser so it recognizes the file extension for downloading.

Firmware FAQs

Go to Tape drive firmware

Go to Library, autoloader, and connectivity solution firmware

## Tape drive firmware

> Important: Do not upgrade tape drive firmware or EEPROM images unless Exabyte Technical Support has advised you to do so. If performed improperly, the upgrade procedure can render your device inoperable. Please consult with Exabyte Technical Support before performing an upgrade. Technical Support will help you select the most appropriate upgrade method for your particular model.

Tape Drive (Which model do I have?) | Latest Firmware | EEPROM Images | Upgrade Methods (Which method should I use?)
--- | --- | --- | ---
Mammoth-2 (M2) |
Important Read this notice before you download firmware for M2!
8ck3v03a - LVD only 8ch3v03a - HVD only | n/a | M2 Monitor (serial or SCSI) Codeload tape
Mammoth and Mammoth-LT | 8cm1v41j
Firmware v40q notice
| 8e000137 - Generic 8e000114 - 8505 emulation 8e000204 - 9600 baud | Mammoth Monitor (serial) EXPERT (SCSI) Codeload tape
Eliant 820 | 8hc-0112 History | 8he-0000 - Generic If you need an EEPROM image with compression off, contact Exabyte Technical Support. | Eliant Monitor (serial) EXPERT (SCSI) Codeload tape
8700 family | 8qc-0052 History | n/a | EXPERT (SCSI) Codeload tape
8505 and 8505XL | 8sc-0808 History | 8se-0010 - Generic 8se-0212 - SCSI enhancement off Misc. - Set of images | CTS Monitor (serial) EXPERT (SCSI) Codeload tape
8205 and 8205XL | 8sc-0808 History | 8ve-0010 - Generic 8ve-0167 - SCSI enhancement off Misc. - Set of images | CTS Monitor (serial) EXPERT (SCSI) Codeload tape
8500c | 8cc-0730 History | 8ce-0010 - Generic 8ce-0201 - SCSI enhancement off Misc. - Set of images | CTS Monitor (serial) EXPERT (SCSI) Codeload tape
8500 | 85c-06x0 History | 85e-0010 - Generic 85e-0155 - SCSI enhancement off Misc. - Set of images | CTS Monitor (serial) EXPERT (SCSI) Codeload tape
8200SX | c034 - Servo History phss261a - MX History | n/a | PROM
8200 | c034 - Servo History prom2644 - MX History | n/a | PROM
4200 and 4200c | Contact Exabyte Technical Support.
2501c | rev73 History | n/a | PROM
2501 | rev29 History | n/a | PROM

### Which upgrade method should I use for my tape drive?

The table above lists the upgrade options available for each model of tape drive. You can review descriptions of each option here. Please consult with Exabyte Technical Support to determine which method is most appropriate for your particular model.

Exabyte Monitor software (using the serial port) | EXPERT for DOS (using the SCSI bus) | Codeload tape | PROM
--- | --- | --- | ---
Use Monitor to upload firmware to your tape drive from an IBM-compatible computer's serial port. The Monitor program for M2 also allows you to upload code across the SCSI bus, if you wish. For all other models, you must purchase a specific serial cable. The Monitor programs for older Exabyte tape drives are DOS based. Mammoth Monitor is available for DOS, Windows 3.1, and Win NT/95. M2 Monitor is available for Windows 95/98/2000/NT 4.0. You can download Monitor free of charge. | Use EXPERT to upload firmware to your tape drive from an IBM-compatible computer across the SCSI bus. No special cable is required. Your computer must be able to run DOS. (Note that EXPERT does not run under the Windows NT 32-bit operating system; you cannot shell to DOS from NT and use EXPERT.) You must also load the appropriate ASPI DOS drivers for the SCSI adapter card installed in your computer. You can download EXPERT free of charge. | Codeload tapes are the easiest way to upload firmware into a tape drive. Your tape drive can be connected to any operating system, and you don't need to shut the system down. You simply insert the codeload tape into the tape drive and the upgrade automatically occurs. You can use the tape as many times as necessary to upgrade drives of the same model. For M2, you can use the codeload tape as a regular data tape after you are finished. You can order a codeload tape from Exabyte Technical Support (overnight delivery is available). | For some of Exabyte's oldest tape drives, the only method of upgrading firmware is to install a new PROM (programmable read-only memory). You can either order a PROM from Exabyte, or create your own by downloading the firmware from this web site and using a PROM burner.

## Library, autoloader, and connectivity solution firmware

> Important: Do not upgrade library, autoloader, or solution firmware unless Exabyte Technical Support has advised you to do so. If performed improperly, the upgrade procedure can render your device inoperable. Please consult with Exabyte Technical Support before performing an upgrade. Technical Support will help you select the most appropriate upgrade method for your particular model.

Library, Autoloader, or Connectivity Solution (Which model do I have?) | Latest Library Firmware | Latest Ethernet Firmware | Upgrade Methods (Which method should I use?)
--- | --- | --- | ---
430 and 110L | 2.2.1 | n/a | Contact Exabyte Technical Support
215 | 2.3.4 | n/a | Contact Exabyte Technical Support
X200, X80, 690D, and 230D | 2.6.3 - Firmware required for M2 support in X200 and X80 History 1.1.2 - Boot code required for M2 support in X200 and X80 | 1.14.2 History | Console interface (serial) WRITE BUFFER (SCSI) FTP (Ethernet)
480, 440, 220, and 210 | 6.5.1 - Firmware required for LVD M2 support 6.4.3 - Firmware required for HVD M2 support | n/a | Console interface (serial) EXPERT (SCSI) WRITE BUFFER (SCSI)
EZ17 | 1.7.4 History | n/a | Console interface (serial) WRITE BUFFER (SCSI)
18D | 2.6.7 History | n/a | Console interface (serial) EXPERT (SCSI) WRITE BUFFER (SCSI)
218 and 018 | 4.13.5 History | n/a | Console interface (serial) EXPERT (SCSI)
10h | 1.11.5 History | n/a | Console interface (serial) EXPERT (SCSI)
120 and 60 | 3.7.57 History | n/a | Console interface (serial) EXPERT (SCSI)
10e | 1.4.5 History | n/a | Console interface (serial) EXPERT (SCSI)
10i | 3.1.24 History | n/a | Console interface (serial) EXPERT (SCSI)
10 | 3.1.40 History | n/a | Console interface (serial) EXPERT (SCSI)
FC11 | e9819e - Enables use of FCX Monitor software | n/a | Configuration interface (serial) FTP (Ethernet)
FC12 | All FC12 routers shipped with the latest firmware and support NetStorM FCX Monitor.

### Which upgrade method should I use for my library, autoloader, or connectivity solution?

The table above lists the upgrade options available for each library, autoloader, and connectivity solution. You can review descriptions of each option here. Please consult with Exabyte Technical Support to determine which method is most appropriate for your particular model.

Console or configuration interface (using the serial port) | EXPERT for DOS (using the SCSI bus) | WRITE BUFFER command (using the SCSI bus) | FTP (using Ethernet)
--- | --- | --- | ---
Most Exabyte libraries and autoloaders have a built-in console interface for upgrading firmware and performing diagnostics. For libraries with an Ethernet interface, you can also upload new Ethernet firmware through the console interface. You can access the console interface by attaching a straight-through 9-pin serial cable to the library's serial port. To communicate with the console interface, use a terminal emulation program such as HyperTerminal or Exabyte's CHS Terminal for DOS, which can be downloaded free of charge. The FC11 also has a serial port that allows you to access internal configuration software and upload firmware. You can use any terminal emulation program that supports XMODEM transfers. | For some Exabyte libraries, you can use EXPERT to upload firmware from an IBM-compatible computer across the SCSI bus. No special cable is required. Your computer must be able to run DOS. (Note that EXPERT does not run under the Windows NT 32-bit operating system; you cannot shell to DOS from NT and use EXPERT.) You must also load the appropriate ASPI DOS drivers for the SCSI adapter card installed in your computer. You can download EXPERT free of charge. On-line help is available with the program, or you can refer to the EXPERT 7 User's Guide, available from the Library of Technical Publications. | For some Exabyte libraries, you can transfer new firmware over the SCSI bus using the WRITE BUFFER command. To use this method, you must have software that can issue SCSI commands directly to the library. For information about the WRITE BUFFER command, refer to the SCSI Reference for your particular library, available from the Library of Technical Publications. | For Exabyte libraries that have an Ethernet interface, you can upload firmware using an Ethernet connection between your computer and the library's Ethernet port. You can also use this method to upgrade the library's Ethernet firmware. The FC11 also has an Ethernet port that you can use for uploading firmware.