
   686 MONITOR  V1.2


> CPU Power-up tests ... passed

> System configuration:
   Memory size (KB)= 1024
   80287 Math Processor.
   Hard Disks   - (1)
> PRESS ANY KEY TO INTERRUPT AUTO-BOOT
> Select [1] to boot from Hard Disk
         [2] to boot from Floppy Disk
         [3] to enter Debugger

> Enter option: 2
> Booting from floppy ...


Concurrent DOS 4.1
Copyright (C) 1985, Digital Research
A>instccpm
686/886 CCP/M-86 Installation Program V1.1
------------------------------------------


Verifying Hard disk number 0
Number of cylinders for this drive = 1024
Number of heads for this drive = 8
Number of sectors per track = 16
Build Bad sector table? [default is Y]
Display bad sector table? [default is Y]

Bad sector address: CYL =  218  HEAD =  1  SEC = 11
Bad sector address: CYL =  301  HEAD =  6  SEC =  8
Bad sector address: CYL =  393  HEAD =  3  SEC =  0
Bad sector address: CYL =  564  HEAD =  2  SEC =  6
Bad sector address: CYL =  878  HEAD =  0  SEC = 10
Bad sector address: CYL = 1023  HEAD =  3  SEC = 13
Number of bad sectors found = 6


Erase hard disk? [default is N] y

Erasing disk:
Track  8191
Floppy drive set to  drive F: Size = 708K,  Dir  = 176
Hard disk 1 logical drive 1 set to  drive A: Size = 32128K,  Dir  = 2048
Hard disk 1 logical drive 2 set to  drive B: Size = 32768K,  Dir  = 2048

Copying files to BOOT tracks
----------------------------
Copy files to hard disk? [default is Y]

Copying files to hard disk
--------------------------
A:MODE    .CMD

Insert disk #2 in floppy drive, Press Any key to continue

Copying files to hard disk
--------------------------
A:XIOS    .DOC

CCP/M-86 Installation Complete, Please reboot the system
A>skipped
> Select [1] to boot from Hard Disk
         [2] to boot from Floppy Disk
         [3] to enter Debugger

> Enter option: 1
> Booting from hard disk ...


Concurrent DOS 4.1
Copyright (C) 1985, Digital Research
A>dir

Directory of Drive A  (CP/M Media)

A: XIOS     CON : CCPM     SYS : ARCHIVE  CMD : VSPAGE   CMD : DCONFIG  CMD
A: SETUP    FIL : PIP      CMD : INSTCCPM CMD : Z80DOWN  FIL : ASM86    CMD
A: VSTV50   CMD : RECOVER  CMD : SIO188   FIL : LOADH886 FIL : VSANSI   CMD
A: LOGV     CMD : VSIMP    CMD : TERM     DAT : VCONFIG  CMD : PRINT    CMD
A: MODE     CMD : BDOS     CON : CIO      CON : MEM      CON : RTM      CON
A: SUP      CON : DIR      CMD : CLOCK    RSP : PCTMP    RSP : PIN      RSP
A: TIME     CMD : SYSTAT   CMD : GENCCPM  CMD : HELP     CMD : ERASE    EXE
A: HELP     HLP : PATCHES  DOC : SYSDISK  CMD : STOP     CMD : PRINTMGR CMD
A: DSP      CMD : SPL      CMD : ERAQ     CMD : SDIR     CMD : SHOW     CMD
A: PATH     EXE : CHSET    CMD : INITDIR  CMD : BATCH    CMD : CHDIR    CMD
A: COPY     EXE : DATE     CMD : MKDIR    CMD : DDT86    CMD : RMDIR    CMD
A: REN      EXE : SET      CMD : SYSDAT   CON : TYPE     CMD : BACKUP   CMD
A: PCONFIG  CMD : RETEN    CMD : PUTSYS   CMD : XCACHE   CMD : DC       CMD
A: MFORMAT  CMD : FTP86    CMD : GEN      IN  : ED       CMD : REN      CMD
A: ERA      CMD : SUBMIT   CMD : TMP      RSP : FPATCH   CMD : XIOS     DOC
        75 File(s) 31690752 bytes free

A>
