README.TXT file for the 64700 Emul/Anly Firmware
------------------------------------------------------------------------
The firmware and the program that downloads it into the HP 64700
are included on the disks labeled "HP64700 Emul/Anly Firmware".  You
only need to load this software if you need to update the firmware 	
for your emulator, analyzer, lan software, or emulator generic 
firmware.  

The firmware revisions of all of the products on this disk are listed
at the end of this README file.  The Real-Time C Debugger requires a 
Version of A.04.00 or higher of the HP64700 generic emulation firmware.
Even though earlier versions of the other subsystems may work, it is
a good idea to use the most recent firmware version available for each
subsystem.

You can check your firmware revisions in the Real-Time C Debugger product
using the Help->About Debugger/Emulator command.  If any of the firmware
is out of date, you should install this utility and update your firmware.

Your HP 64700 must contain Flash EPROM memory before you can update
HP 64700 system firmware.  If it does not, you must contact your
HP field representative in order to update your ROMS.

Instructions for updating the firmware can be found in the Real-Time
C manual chapter "Installing/Updating HP 64700 Firmware".

Installation
------------
1.  To install the 64700 Firmware Update Utility, start MS Windows.
    Insert the "HP64700 Emul/Anly Firmware 1 of 2" disk into
    the floppy disk drive a or b.  

    Choose the File->Run command in the Windows Program Manager.
    Enter "b:setup" or "c:setup" in the Command Line text box.

    You will be asked to enter a path for the utility, or use the
    default HP64700 path.  All of the firmware files will be copied
    to your hard disk.

2.  After the Setup Program has completed, if you installed the files
    in a location other than the default HP64700, you must set the
    HP64700 and HPTABLES environment variables.  These variables are
    used by PROGFLASH.EXE to find the required files.  You will probably
    want to place commands to set these variables into your 'autoexec.bat'
    file for execution on boot up.

    - Set the environment variable HP64700 to the directory where you
      installed the utility.  
      For example:  set  HP64700=A:\HP64700 

    - The environment variable HPTABLES must be assigned the path name
      of the TABLES directory, this path will always be the TABLES 
      subdirectory of your path.
      For example:  set  HPTABLES=A:\HP64700\TABLES

    - The FLASH.BAT file in the BIN directory must be modified to use
      the path where you installed the utility.

3.  Modify your 'config.sys' file to contain the following lines:

    BREAK=ON
    FILES=20

4.  If you do not already have an emulator device table file (64700TAB)
    that you have set up and want to keep, edit the default device table
    A:\HP64700\TABLES\64700TAB to reflect your hardware configuration.
    The default table contains entries for COM1 and COM2 at 9600 Baud.


5.  Select the "PROGFLASH" icon in the HP64700 Firmware Update Utility 
    Program Manager Group to run the utility.




************************************************************************

                      Firmware Versions on this disk

************************************************************************
64700       A.04.02 GENERIC EMULATION                        29Jan96                       
64700B      A.05.06 GENERIC EMULATION                        29Jan96                     
64701A      A.00.07 LAN
64701A      A.00.07 LAN FIRMWARE                   64701     10Feb94                      
64705A      A.00.02 ANALYSIS FIRMWARE              64705     06Jan94                      
64740       A.02.03 TRACE ANALYZER                           10Jan94                      
64742A      A.00.10 68000 DIP EMULATOR 128K                  10Jan94                      
64743A      A.00.04 68000 16MHz EMULATOR                     10Jan94                      
64744A      A.00.04 68EC000 EMULATION FIRMWARE     64744     04Mar94                       
64794A      A.03.03 DEEP EMULATION ANALYZER                  23Aug95                     
64700AX008  A.00.05 64700 SW UTIL                            01Mar94                       
