
***********************************************************
*                                                         *
*  HP 64000 Software CD-ROM for DOS, Windows, Windows95,  *
*  and WindowsNT -- Software Installation Guide           *
*                                                         *
***********************************************************


About the HP 64000 Software CD-ROM
==================================


Installation Media Contains other Installation Media
----------------------------------------------------

The HP 64000 software CD-ROM is different from other
software media CD-ROMs in that it contains many individual
products *and* their installation programs.  It's a
collection of the installation media for all HP 64000
PC products.

When you install software from this CD-ROM, you extract
a product's installation media; then, you can install
the product as if you were installing from the product's
floppy disks, or you can make copies of a product's
installation media and place them on floppy disks.


Restricted Paths Through the SETUP Program
------------------------------------------

Because of the number of products on this CD-ROM, little
backtracking is allowed in the SETUP program.  So, it's
important to understand the selections you will make.

If you make a wrong choice during the installation, you
may have to cancel SETUP and perform the installation
again.


Passwords Required for Some Products
------------------------------------

Passwords are required to install some of the products
on this CD-ROM.  Installation passwords are found on the
Software Certificate received when a product license is
purchased.


Product Version Information
---------------------------

Version information for the products contained on this
CD-ROM can be found in the PRODREV.TXT file.


Installation Notes on CD-ROM
----------------------------

These installation notes are also included on the CD-ROM
in an ASCII file named INSTALL.TXT.


Installation Notes
==================

Installation instructions and system requirements are
printed on the CD-ROM package.  (Basically, insert the
HP 64000 Software CD-ROM disk into your drive and run
the SETUP program.)

Once the SETUP program is running, follow its instructions
and select from the options it presents.

This document provides additional notes on the setup
and installation process, including descriptions of:

 * Platform selection
 * Types of installations
 * Types of products
 * Passwords
 * Selecting products
 * Individual product installations
 * Finishing the installation


Platform Selection
------------------

Platform selection specifies the type of PC (that is,
IBM or NEC) you're installing software on.

If you're using DOS/V (a Japanese localized operating
system), select IBM-PC compatible.


Types of Installations
----------------------

You choose the following types of installations:

 * You can install new products on your PC.

 * You can update products or firmware that already exist
   on your PC.

 * You can create the installation media floppies for
   a product.


Types of Products
-----------------

You can choose from the following types of products:

 * Windows-based Real-Time C Debugger products

 * Windows-based C Debug User Interfaces (Netrap)

 * 68000 Family Cross Compiler/Assemblers

 * Windows-based Software Analyzer or Processor Probe
   interfaces

   Win32s must be installed before you can install the
   HP B3740A Software Analyzer and HP B3745A MIPS Processor
   Probe interface products.  If Win32s is not already
   installed on your PC, you can get it from the CD-ROM
   -- see the \RTCS\WIN32S\DISK1 directory.

 * DOS-based emulator user interfaces

 * Flash update programs and firmware


-- Flash Update Programs and Firmware --

When installing, updating, or creating media floppies for
flash update programs or emulator firmware, you can choose
from four categories:

 * Flash update program for LAN connections

   This is a *new* flash update program that works for
   emulators or processor probes connected to the PC via
   LAN.  This program runs on Windows95 or WindowsNT.

 * Flash update program for RS-232 connections

   This is the original flash update program that works
   for emulators connected to the PC via RS-232.  This
   program runs on DOS or Windows 3.1.

 * Firmware for flash updates

   Provides a list of all the emulator firmware products
   from which you can select individual firmware products
   to install/update.

 * Flash update program and firmware

   This is the traditional, floppy-disk packaged flash
   update program (for RS-232) and emulator firmware.


Passwords
---------

If a password is required, the SETUP program will prompt
you for it.

Installation passwords can be found on the Software
Certificate received when a software product license
is purchased.

You don't have to include spaces when typing in the
password, but you can leave them in for readability.


Selecting Products
------------------

You must check the boxes of the products you wish to
install.  (Highlighting a line does not select it.)

If you select multiple products, note the amount of disk
space required (listed in the upper right-hand corner of
the product selection dialog).  The SETUP program checks
for disk space as individual products are installed; it
does not check for the total amount of disk space required.


Individual Product Installations
--------------------------------

After a selected product is unlocked and de-compressed
(that is, after the installation media is placed in a
temporary location), the setup program for that product
is automatically run.

Follow the instructions in that product's setup program,
and refer to that product's software installation
documentation for more information.

Note that after individual product installations are
complete, the main CD-ROM setup program is still running.
You may have to minimize other windows to select the
setup window again.


Finishing the Installation
--------------------------

When the installation has completed, you will be notified
that installation may require a re-boot of your computer.
You have the option of re-booting automatically or
rebooting yourself later.  After you've made your
selection, click the Finish button.

