*********************************************************
*M*      VDCB     VIRTUAL MEMORY PARTITION DEFINITIONS FOR LINK
*********************************************************
*P*      NAME:    VDCB
*P*      PURPOSE: TO DEFINE THE PARTITIONS IN THE USER'S SPACE
*P*               WHERE LINK WILL BUILD THE VARIOUS PROTECTION
*P*               TYPE AREAS OF A LOAD MODULE.
*P*      DESCRIPTION: VDCB DEFINES THE BOUNDARIES OF THE FIXED
*P*               PARTITIONS IN THE USER'S VIRTUAL SPACE WHERE
*P*               LINK WILL BUILD A LOAD MODULE'S DATA, DCBS,
*P*               AND PROCEDURE.
***************************************************************
 ASECT
         DEF      VDCB              THE START OF THE DCB AREA IN A
*,*                                 LINK-BUILT LOAD MODULE.
*,*                                 VDCB MUST BE X'400' WORDS LESS
*,*                                 THAN VPP.
         DEF      VLC               THE START OF THE DATA AREA FOR A
*,*                                 LINK-BUILT LOAD MODULE.
         DEF      VPP               THE START OF THE PROCEDURE AREA FOR
*,*                                 A LINK-BUILT LOAD MODULE
         DEF      VDP               THE END OF THE AVAILABLE USER AREA
*,*                                 IN A LINK-BUILT LOAD MODULE.
VDCB ORG X'16C00'
VLC ORG X'A000'
VPP ORG X'17000'
VDP ORG X'1C000'
 END

