IMageDisk Analyzer 1.20 / Jan 09 2024
IMD 1.17: 17/07/2009 17:46:52

Televideo TS 803H Boot/Utility Disk

Required cylinders: 40
Required heads    : 2
Data rate         : 250kbps
Est. maximum track: 6223 bytes

Possible drives/options to write 803HBOOT.IMD :

 5.25" DD 40-track
   Double-step: OFF

 5.25" QD 80-track
   Double-step: ON

 5.25" HD 80-track
   Double-step: ON
   250 kbps -> 300 kbps

 3.5" DD 80-track   NOTE: *1
   Double-step: OFF

 3.5" HD 80-track   NOTE: *1
   Double-step: OFF

*1 40 track image will use only first 1/2 of 80-track drive.



IMageDisk Utility 1.20 / Jan 09 2024
IMD 1.17: 17/07/2009 17:46:52

Televideo TS 803H Boot/Utility Disk

Assuming 1:1 for Binary output
 0/0 250 kbps DD  18x256
      1   4   7   10  13  16  2   5   8   11  14  17  3   6   9   12  15  18 
      D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 0/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 1/0  D   D   D   D   DE5 DE5 D   D   D   DE5 DE5 DE5 D   D   D   DE5 DE5 DE5
 1/1  DE5 DE5 DE5 D   D   D   DE5 DE5 DE5 D   D   D   DE5 DE5 DE5 D   D   DE5
 2/0  D   D   DE5 D   D00 D   D   D   DE5 D   D00 D   D   D   D   D00 D00 D  
 2/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 3/0  D   D   D00 D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 3/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 4/0  D   D   DE5 D   D   D   D   D   DE5 D   D   D   D   DE5 D   D   D   D  
 4/1  D   D   D   D   DE5 D   D   D   D   D   DE5 D00 D   D   D   DE5 D   D00
 5/0  D00 D00 D00 D   D   D   D00 D00 D   D   D   D   D00 D00 D   D   D   D  
 5/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 6/0  D   D   D   D   DE5 DE5 D   D   D   D   DE5 D   D   D   D   DE5 DE5 D  
 6/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 7/0  D   D   DE5 DE5 D   D   D   D   DE5 DE5 D   D   D   D   DE5 DE5 D   DE5
 7/1  DE5 D   DE5 DE5 D   DE5 DE5 D   DE5 D   D   DE5 D   DE5 DE5 D   D   DE5
 8/0  D   D   D   DE5 DE5 DE5 D   D   DE5 DE5 DE5 D   D   D   D   DE5 DE5 D  
 8/1  D   D   D   D   D   D00 D   D   D   D   D   D00 D   D   D   D   D00 D00
 9/0  D00 D00 D00 D00 D00 D00 D00 D00 D00 D00 D00 D00 D00 D00 D00 D00 D00 D00
 9/1  D00 D00 D   D   D   D   D00 D00 D   D   D   D   D00 D00 D   D   D   D  
10/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
10/1  D   D00 D00 D00 D00 D00 D   D00 D00 D00 D00 D00 D   D00 D00 D00 D00 D00
11/0  D00 D00 D00 D00 D   D   D00 D00 D00 D00 D   D   D00 D00 D00 D   D   DE5
11/1  DE5 D   D   D   D   D   DE5 D   D   D   D   D   D   D   D   D   D   D  
12/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
12/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
13/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
13/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
14/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
14/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
15/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
15/1  D   D   DE5 DE5 DE5 DE5 D   D   DE5 D   DE5 DE5 D   DE5 DE5 DE5 DE5 DE5
16/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
16/1  D   D   D   DE5 DE5 D   D   D   D   DE5 DE5 D   D   D   DE5 DE5 D   D  
17/0  D   DE5 DE5 DE5 D   D   D   D   DE5 DE5 D   D   DE5 D   DE5 DE5 D   D  
17/1  DE5 D   D   D   D   D   DE5 D   D   D   D   D   D   D   D   D   D   D  
18/0  D   D   D00 D00 D   D   D   D   D00 D00 D   D   D   D00 D00 D   D   D00
18/1  D00 D00 D   D   DE5 D   D00 D00 D   D   DE5 D   D00 D00 D   D   D   D  
19/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
19/1  D   D   D   D   D   DE5 D   D   D   D   DE5 DE5 D   D   D   D   DE5 DE5
20/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
20/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
21/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
21/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
22/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
22/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
23/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
23/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
24/0  D   D   D   D   DE5 DE5 D   D   D   D   DE5 D   D   D   D   DE5 DE5 D  
24/1  D   D   D   D   D   D   D   DE5 D   D   D   D   D   DE5 D   D   D   D  
25/0  D   D   D   D   D   D   D   D   D   D   D00 D   D   D   D   D   D   D  
25/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
26/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
26/1  D   D   D   D   D   D   D   D   D   D   D   DE5 D   D   D   D   D   DE5
27/0  DE5 DE5 D   D   D   DE5 DE5 D   D   D   D   DE5 DE5 D   D   D   DE5 DE5
27/1  DE5 D   D   D   D   D   DE5 D   D   D   D   D   D   D   D   D   D   D  
28/0  D   D   D   D   DE5 DE5 D   D   D   DE5 DE5 D   D   D   D   DE5 DE5 D  
28/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
29/0  D   D   D   D   D   DE5 D   D   D   D   DE5 DE5 D   D   D   D   DE5 DE5
29/1  DE5 D   D   DE5 DE5 DE5 DE5 D   DE5 D   DE5 DE5 D   D   DE5 D   DE5 DE5
30/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
30/1  D   D   D   DE5 DE5 D   D   DE5 D   DE5 DE5 D   D   DE5 D   DE5 D   D  
31/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
31/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
32/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
32/1  D   D   D   D   D   D   D   D   D   D   DE5 D   D   D   D   D   D   D  
33/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
33/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
34/0  D   DE5 DE5 D   D   D   D   DE5 DE5 D   D   D   D   DE5 D   D   D   D  
34/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
35/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
35/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
36/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
36/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
37/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
37/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
38/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
38/1  D   D   D   D   D   D   D   D   D   D   D   D   D   DE5 D   D   D   D  
39/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
39/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
80 tracks(40/40), 1440 sectors (231 Compressed)



BEGIN TEL4  TeleVideo 8nn-TPC-1 CP/M - DSDD 48 tpi 5.25" - 256 x 18
DENSITY MFM, LOW
CYLINDERS 40 SIDES 2 SECTORS 18,256 SKEW 6
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
ORDER CYLINDERS
BSH 4 BLM 15 EXM 0 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END

# TEL4  TeleVideo 8nn/TPC-1 CP/M - DSDD 48 tpi 5.25" - 256 x 18
diskdef tel4
  seclen 256
  tracks 80
  sectrk 18
  blocksize 2048
  maxdir 64
  skew 1
#  boottrk 4
  offset 18432
  boottrk 0
  os 2.2
end

# libdsk
[tel4]
description = TEL4  TeleVideo 8nn/TPC-1 CP/M - DSDD 48 tpi 5.25" - 256 x 18
sides = outback
cylinders = 80
heads = 2
secsize = 256
sectors = 18
secbase = 1
datarate = DD

# Flashfloppy/GOTEK
[tel4]
cyls = 80
heads = 2
secs = 18
interleave = 1
bps = 256
id = 1
#rpm = 360
rpm = 300
rate = 250
mode = mfm
iam = no



Directory is at 0x4800 = 18432 Decimal
00004800   00 4D 4F 56  43 50 4D 20  20 43 4F 4D  00 00 00 50  .MOVCPM  COM...P
00004810   01 02 03 04  05 00 00 00  00 00 00 00  00 00 00 00  ................
00004820   00 50 49 50  20 20 20 20  20 43 4F 4D  00 00 00 3A  .PIP     COM...:
00004830   06 07 08 09  00 00 00 00  00 00 00 00  00 00 00 00  ................
00004840   00 53 54 41  54 20 20 20  20 43 4F 4D  00 00 00 29  .STAT    COM...)
00004850   0A 0B 0C 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
00004860   00 41 53 4D  20 20 20 20  20 43 4F 4D  00 00 00 40  .ASM     COM...@
00004870   0D 0E 0F 10  00 00 00 00  00 00 00 00  00 00 00 00  ................
00004880   00 44 44 54  20 20 20 20  20 43 4F 4D  00 00 00 26  .DDT     COM...&
00004890   11 12 13 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
000048A0   00 45 44 20  20 20 20 20  20 43 4F 4D  00 00 00 34  .ED      COM...4
000048B0   14 15 16 17  00 00 00 00  00 00 00 00  00 00 00 00  ................
000048C0   00 53 55 42  4D 49 54 20  20 43 4F 4D  00 00 00 0A  .SUBMIT  COM....
000048D0   18 00 00 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
000048E0   00 58 53 55  42 20 20 20  20 43 4F 4D  00 00 00 06  .XSUB    COM....
000048F0   19 00 00 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
00004900   00 53 59 53  47 45 4E 20  20 43 4F 4D  00 00 00 09  .SYSGEN  COM....
00004910   1A 00 00 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
00004920   00 4C 4F 41  44 20 20 20  20 43 4F 4D  00 00 00 0E  .LOAD    COM....
00004930   1B 00 00 00  00 00 00 00  00 00 00 00  00 00 00 00  ................
00004940   00 50 41 52  4B 20 20 20  20 43 4F 4D  00 00 00 02  .PARK    COM....
00004950   1C 00 00 00  00 00 00 00  00 00 00 00  00 00 00 00  ................



$ cpmls -f tel4 -T rawob -D 803HBOOT.RAW
     Name    Bytes   Recs  Attr     update             create
------------ ------ ------ ---- -----------------  -----------------
803HDEMO.COM    26K    208    
ASM     .COM     8K     64    
ASSIGN  .SYS     2K      1    
BUILDDSK.SUB     2K      4    
COPYDISK.COM    22K    163    
DD7220  .PRL    10K     80    
DD7470  .PRL    12K     86    
DDHI3M  .PRL    10K     69    
DDHI7M  .PRL    10K     80    
DDMX80  .PRL    12K     92    
DDT     .COM     6K     38    
DDTS803 .PRL     8K     51    
DEMOSCRN.        2K      5    
DEMOTXT2.BIN    10K     65    
DUMP    .COM     2K      4    
ED      .COM     8K     52    
FIXDISK .COM     2K      9    
FORMAT  .COM    28K    218    
GENGRAF .COM     2K     12    
GSX     .SYS     2K     11    
GSXREAD .ME      6K     43    
HFORMAT .COM     4K     20    
LOAD    .COM     2K     14    
MOVCPM  .COM    10K     80    
PARK    .COM     2K      2    
PIP     .COM     8K     58    
SETUP   .COM     8K     52    
STAT    .COM     6K     41    
SUBMIT  .COM     2K     10    
SURF1   .       20K    150    
SYSGEN  .COM     2K      9    
TOD     .COM     2K     11    
XSUB    .COM     2K      6    
   33 Files occupying    258K,     100K Free.



