IMageDisk Analyzer 1.20 / Jan 09 2024
IMD 1.17: 17/07/2009 17:04:29

Televideo TS 803 Telecalc/Telechart 80 v1.0

Required cylinders: 40
Required heads    : 2
Data rate         : 250kbps
Est. maximum track: 6223 bytes

Possible drives/options to write TCHART.IMD :

 5.25" DD 40-track
   Double-step: OFF

 5.25" QD 80-track
   Double-step: ON

 5.25" HD 80-track
   Double-step: ON
   250 kbps -> 300 kbps

 3.5" DD 80-track   NOTE: *1
   Double-step: OFF

 3.5" HD 80-track   NOTE: *1
   Double-step: OFF

*1 40 track image will use only first 1/2 of 80-track drive.



IMageDisk Utility 1.20 / Jan 09 2024
IMD 1.17: 17/07/2009 17:04:29

Televideo TS 803 Telecalc/Telechart 80 v1.0

Assuming 1:1 for Binary output
 0/0 250 kbps DD  18x256
      4   7   10  13  16  2   5   8   11  14  17  3   6   9   12  15  18  1  
      DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
 0/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
 1/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
 1/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
 2/0  DE5 DE5 D   D   D   D   DE5 DE5 D   D   D   D   DE5 D   D   D   D   D  
 2/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 3/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 3/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   DE5 D  
 4/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 4/1  D   D   D   D   D   D   D   D   D   DE5 D   D   D   D   D   D   D   D  
 5/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 5/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 6/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 6/1  D   D   D   D   D   D   D   D   D   D   DE5 D   D   D   D   D   DE5 D  
 7/0  DE5 D   D   D   D   DE5 D   D   D   D   D   DE5 D   D   D   D   D   DE5
 7/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 8/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 8/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 9/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
 9/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
10/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
10/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
11/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
11/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
12/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
12/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
13/0  D   DE5 DE5 D   D   D   D   DE5 DE5 D   DE5 D   DE5 DE5 DE5 D   DE5 D  
13/1  D   D   D   D   D   DE5 D   D   D   D   D   D   D   D   D   D   D   DE5
14/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
14/1  D   D   D   DE5 D   D   D   D   DE5 DE5 D   D   D   D   DE5 D   D   D  
15/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
15/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
16/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
16/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
17/0  DE5 D   D   D   D   D   D   D   D   D   D   DE5 D   D   D   D   D   D  
17/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
18/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
18/1  D   D   D   DE5 DE5 D   D   D   D   DE5 DE5 D   D   D   D   D   DE5 D  
19/0  DE5 D   D   D   D   DE5 D   D   D   D   D   DE5 D   D   D   D   D   DE5
19/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
20/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
20/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
21/0  D   DE5 DE5 D   D   D   D   DE5 DE5 D   D   D   D   DE5 DE5 D   D   D  
21/1  D   D   D   D   D   DE5 D   D   D   D   D   D   D   D   D   D   D   D  
22/0  DE5 DE5 D   D   D   DE5 DE5 DE5 D   D   D   DE5 DE5 D   D   D   D   D  
22/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
23/0  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
23/1  D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D   D  
24/0  DE5 DE5 D   DE5 DE5 D   DE5 DE5 D   DE5 DE5 D   DE5 D   DE5 DE5 DE5 D  
24/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
25/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
25/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
26/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
26/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
27/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
27/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
28/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
28/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
29/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
29/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
30/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
30/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
31/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
31/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
32/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
32/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
33/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
33/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
34/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
34/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
35/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
35/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
36/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
36/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
37/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
37/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
38/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
38/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
39/0  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
39/1  DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5 DE5
80 tracks(40/40), 1440 sectors (695 Compressed)



BEGIN TEL4  TeleVideo 8nn-TPC-1 CP/M - DSDD 48 tpi 5.25" - 256 x 18
DENSITY MFM, LOW
CYLINDERS 40 SIDES 2 SECTORS 18,256 SKEW 6
SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
ORDER SIDES
BSH 4 BLM 15 EXM 0 DSM 170 DRM 63 AL0 080H AL1 0 OFS 4
END

# TEL4  TeleVideo 8nn/TPC-1 CP/M - DSDD 48 tpi 5.25" - 256 x 18
diskdef tel4
  seclen 256
  tracks 80
  sectrk 18
  blocksize 2048
  maxdir 64
  skew 1
  boottrk 4
  os 2.2
end

# libdsk
[tel4]
description = TEL4  TeleVideo 8nn/TPC-1 CP/M - DSDD 48 tpi 5.25" - 256 x 18
sides = alt
cylinders = 80
heads = 2
secsize = 256
sectors = 18
secbase = 1
datarate = DD

[tel4]
cyls = 80
heads = 2
secs = 18
interleave = 1
bps = 256
id = 1
#rpm = 360
rpm = 300
rate = 250
mode = mfm
iam = no



$ cpmls -f tel4 -D TCHART.RAW
     Name    Bytes   Recs  Attr     update             create
------------ ------ ------ ---- -----------------  -----------------
PRINTER .COM    16K    123    
PRINTER .SET     2K      2    
TC      .COM    18K    139    
TCCHTOPT.OVL    12K     88    
TCERROR .FIL     6K     33    
TCFORM  .OVL    18K    143    
TCHELP  .FIL    20K    148    
TCLOGIC .OVL    20K    147    
TCMENU  .FIL     2K     14    
TCPRINT .OVL    20K    145    
TCPRNT  .OVL     2K     15    
TCSBAR  .OVL    16K    125    
TCSET   .OVL     2K      8    
TCSETUP .FIL     2K      6    
TCSHOW  .OVL    18K    143    
TCSPIE  .OVL     8K     61    
TCSTAT  .OVL    18K    134    
   17 Files occupying    200K,     140K Free.



