{
A
|DESCRIPTION|Epson GQ-3500 Laser Printer (300 x 300 Dots/Inch)
|SHORT DESCR|EPSON GQ 3500
|FILENAME|PDEGH8.B30
|AUX FILE|EGH.ATM
|FNT WILDCRD|*.B30
|LONG DESCRP|
Choose this entry if you are using the Epson GQ-3500 Laser 
printer.  This printer offers a print resolution of 300 x 300 
dots per inch. 
}
{
B
|DESCRIPTION|Epson LQ Series Printers (180 x 180 Dots/Inch)
|SHORT DESCR|Epson LQ
|FILENAME|PDELQ8.ELQ
|AUX FILE|ELQ.ATM
|FNT WILDCRD|*.ELQ
|LONG DESCRP|
Choose this entry if you are using an Epson LQ-Series printer.  
LQ-Series printers offer a print resolution of 180 x 180 
dots per inch.
}
{
C
|DESCRIPTION|Hewlett Packard Laserjet II Printer (300 x 300 Dots/Inch)
|SHORT DESCR|HP Laser II
|FILENAME|PDHPU8.B30
|FNT WILDCRD|*.B30
|LONG DESCRP|
Choose this entry if you are using a Hewlett Packard Laserjet 
II printer.  This printer offers a print resolution of 300 x 300 
dots per inch.
}
{
D
|DESCRIPTION|Hewlett Packard LaserJet+ (150 x 150 Dots/Inch)
|SHORT DESCR|HP Laserjet+
|FILENAME|PDHPH8.HPH
|FNT WILDCRD|*.HPH
|LONG DESCRP|
Choose this entry if you are using a Hewlett Packard LaserJet+ 
printer.  This printer offers a resolution of 150 x 150 dots per 
inch. 
}
{
E
|DESCRIPTION|IBM/Epson High Resolution Printers (120 x 144 Dots/Inch)
|SHORT DESCR|IBM/Epson Hi
|FILENAME|PDEHI8.EPS
|AUX FILE|EHI.ATM
|FNT WILDCRD|*.EPS
|LONG DESCRP|
Choose this entry if you are using an IBM Graphics printer, the 
Epson FX 80/100, or the Epson MX 80/100.  These printers offer a
resolution of 120 x 144 dots per inch. 
}
{
F
|DESCRIPTION|IBM Proprinter (120 x 144 Dots/Inch)
|SHORT DESCR|Proprinter
|FILENAME|PDPRO8.EPS
|AUX FILE|PRO.ATM
|FNT WILDCRD|*.EPS
|LONG DESCRP|
Choose this entry if you are using the IBM Proprinter.  This printer 
offers 120 x 144 dots per inch print resolution. 
}
{
G
|DESCRIPTION|LaserWriter / Postscript Printers
|SHORT DESCR|Postscrpt 12
|FILENAME|PDPST8.SYS
|AUX FILE|PSTV23.PRE;PSTV23.CNF
|LONG DESCRP|
Choose this entry if you are using a printer that uses Postscript-type 
files and the standard Adobe resident font set: Courier, Helvetica, 
Times, and Symbol.
}
{
H
|DESCRIPTION|LaserWriter Plus / Postscript Printers
|SHORT DESCR|Postscrpt 35
|FILENAME|PDPST8.SYS
|AUX FILE|PST.PRE;PST.CNF
|LONG DESCRP|
Choose this entry if you are using a printer that uses 
Postscript-type files and has the extended Adobe resident font 
set: Bookman, Zapf-Chancery, etc. in addition to the standard
resident font set: Courier, Helvetica, Times, and Symbol.
}
{
I
|DESCRIPTION|Toshiba P321, P341, or P351 Printer (180 x 180 Dots/Inch)
|SHORT DESCR|Toshiba
|FILENAME|PDTSH8.ELQ
|AUX FILE|TSH.ATM
|FNT WILDCRD|*.ELQ
|LONG DESCRP|
Choose this entry if you are using a Toshiba 321,341, or 351 
printer.  Each of these printers offers a print resolution of 180 
x 180 dots per inch.
}
