
		    +------------------------------+
		    |	TMS320C30 APPLICATION	   |
		    |		BOARD		   |
		    |	      Version 1.1	   |
		    |	     Release Notes	   |
		    +------------------------------+


   This file contains release notes for Version 1.1 of the TMS320C30
   Application Board.  Plese read this documentation carefully before you
   install the package.

   The TMS320C30 Application Board software is shipped on one floppy diskette.
   The following is a list of the files contained on the floppy
   diskette:


	FILE			     DESCRIPTION
   ==============      ===================================================

    INIT.CFM		A command file which defines the default memory
			configuration of TMS320C30 Application Board.

    INIT.IOB		A file that defines the I/O memory block in which
			the TMS320C30 Emulator will operate.

    RESVCT.001		TMS320C30A reset vector file used by the TMS320C30
			Emulator.

    RESVCT.002		TMS320C30B reset vector file used by the TMS320C30
			Emulator.

    C30RESET.EXE	The execution file which is used to reset TMS320C30
			Application Board.

    C30EXAM.ASM 	TMS320C30 sample assembly program.

    C30EXAM.CMD 	Link command file for C30EXAM.ASM.

    C30EXAM.OUT 	COFF object file for C30EXAM.ASM.

    README		This file.

DIFFERENCES FROM RELEASE 1.0
=============================

    1.	The file reset2.vct was renamed resvct.001.

    2.	The file resvct.002 was added.

    3.	The file c30exam.exe was modified to make more efficent use of
	DRAM and enable the cache during program execution.



