File: pef/c9 3550_dual_nonboot 2.pef

     Data Fork Container (length 0x6BC0/27584)

     Container Header
0000 magic1, magic2   = 0x4A6F7921 ('Joy!')
0004 containerID      = 0x70656666 ('peff')
0008 architectureID   = 0x70777063 ('pwpc')
000C versionNumber    = 0x00000001 (1)
0010 dateTimeStamp    = 0xB989206F (Wed Aug 21 03:48:15 2002)
0014 oldDefVersion    = 0x00000000 (0)
0018 oldImpVersion    = 0x00000000 (0)
001C currentVersion   = 0x00000000 (0)
0020 nbrOfSections    = 3
0022 loadableSections = 2
0024 memoryAddress    = 0x00000000

     =========================================================

     Section Header 0
0028 sectionName      = 0xFFFFFFFF (-1) ... <unnamed>
002C sectionAddress   = 0x00000000
0030 execSize         = 0x00004D00 (19712)
0034 initSize         = 0x00004D00 (19712)
0038 rawSize          = 0x00004D00 (19712)
003C containerOffset  = 0x000004B0 (1200)
0040 regionKind       = 0x00       (code)
0041 shareKind        = 0x04       (global share)
0042 alignment        = 0x04       (16-byte bndry)
0043 reserved         = 0x00

     Section Header 1
0044 sectionName      = 0xFFFFFFFF (-1) ... <unnamed>
0048 sectionAddress   = 0x00000000
004C execSize         = 0x00001A10 (6672)
0050 initSize         = 0x00001A10 (6672)
0054 rawSize          = 0x00001A10 (6672)
0058 containerOffset  = 0x000051B0 (20912)
005C regionKind       = 0x01       (data)
005D shareKind        = 0x04       (global share)
005E alignment        = 0x04       (16-byte bndry)
005F reserved         = 0x00

     Section Header 2
0060 sectionName      = 0xFFFFFFFF (-1) ... <unnamed>
0064 sectionAddress   = 0x00000000
0068 execSize         = 0x00000000 (0)
006C initSize         = 0x00000000 (0)
0070 rawSize          = 0x0000042A (1066)
0074 containerOffset  = 0x00000080 (128)
0078 regionKind       = 0x04       (loader)
0079 shareKind        = 0x04       (global share)
007A alignment        = 0x04
007B reserved         = 0x00

007C There are 4 (pad?) bytes at the end of the section headers.
     This is probably because there's no string table.

     =========================================================

     Loader section 2 (<unnamed>)

     ------- Loader Header -------
0080 entrySection     = 0x00000001 (1)
0084 entryOffset      = 0x00000148 (328)
0088 initSection      = 0x00000001 (1)
008C initOffset       = 0x00000150 (336)
0090 termSection      = 0x00000001 (1)
0094 termOffset       = 0x00000140 (320)
0098 nbrImportIDs     = 0x00000004 (4)
009C nbrImportSyms    = 0x0000001E (30)
00A0 nbrRelocSects    = 0x00000001 (1)
00A4 relocsOffset     = 0x0000011C (284)
00A8 strTblOffset     = 0x00000140 (320)
00AC slotTblOffset    = 0x000003D4 (980)
00B0 hashSlotTblSz    = 0x00000002 (2) [==> 4]
00B4 nbrExportSyms    = 0x00000005 (5)

     ------ Loader Import Symbol Table ------
          Importing from "DriverServicesLib ; oldImpVersion 0x00000000 (0), currentVersion 0x00000000 (0)"
0118 [ 0] 82 000036 w TVector  AddDevicePowerHandler
011C [ 1] 82 00004C w TVector  PBQueueInit
0120 [ 2] 82 000058 w TVector  PBQueueCreate
0124 [ 3] 82 000066 w TVector  InstallInterruptFunctions
0128 [ 4] 82 000080 w TVector  DelayForHardware
012C [ 5] 82 000091 w TVector  PrepareMemoryForIO
0130 [ 6] 82 0000A4 w TVector  PoolAllocateResident
0134 [ 7] 82 0000B9 w TVector  NanosecondsToAbsolute
0138 [ 8] 82 0000CF w TVector  DecrementAtomic
013C [ 9] 82 0000DF w TVector  CheckpointIO
0140 [10] 82 0000EC w TVector  MemAllocatePhysicallyContiguous
0144 [11] 82 00010C w TVector  CStrNCat
0148 [12] 82 000115 w TVector  IOCommandIsComplete
014C [13] 82 000129 w TVector  GetLogicalPageSize
0150 [14] 82 00013C w TVector  PoolDeallocate
0154 [15] 82 00014B w TVector  CStrNCopy
0158 [16] 82 000155 w TVector  SetDevicePowerLevel
015C [17] 82 000169 w TVector  BlockCopy
0160 [18] 82 000173 w TVector  GetInterruptFunctions

          Importing from "NameRegistryLib ; oldImpVersion 0x00000000 (0), currentVersion 0x00000000 (0)"
0164 [19] 02 000189   TVector  RegistryEntryIDCopy
0168 [20] 02 00019D   TVector  RegistryPropertyGet
016C [21] 02 0001B1   TVector  RegistryPropertyGetSize

          Importing from "PCILib ; oldImpVersion 0x00000000 (0), currentVersion 0x00000000 (0)"
0170 [22] 02 0001C9   TVector  EndianSwap32Bit
0174 [23] 02 0001D9   TVector  EndianSwap16Bit
0178 [24] 02 0001E9   TVector  ExpMgrConfigWriteWord

          Importing from "InterfaceLib ; oldImpVersion 0x00000000 (0), currentVersion 0x00000000 (0)"
017C [25] 02 0001FF   TVector  SCSIReregisterBus
0180 [26] 02 000211   TVector  LockMemory
0184 [27] 02 00021C   TVector  NewRoutineDescriptor
0188 [28] 02 000231   TVector  SCSIRegisterBus
018C [29] 02 000241   TVector  CallUniversalProc

     ------ Loader Relocation Headers ------
0190 [0] sectionNumber    = 1
0192     reserved         = 0x0000
0194     nbrOfRelocs      = 17
0198     firstRelocInstr  = 0x00000000 (0)

     ------ Loader Relocation Instructions ------
          Relocations for section 1 (<unnamed>)
          Instr     Op    Operand           codeA dataA rSymI rAddr
019C [ 0] 4A1D      SYMR  cnt=30              0     1     0   00000000
019E [ 1] 4210      DATA  cnt=17              0     1    30   00000078
01A0 [ 2] 4003      CODE  cnt=4               0     1    30   000000BC
01A2 [ 3] 4200      DATA  cnt=1               0     1    30   000000CC
01A4 [ 4] 4002      CODE  cnt=3               0     1    30   000000D0
01A6 [ 5] 4206      DATA  cnt=7               0     1    30   000000DC
01A8 [ 6] 4001      CODE  cnt=2               0     1    30   000000F8
01AA [ 7] 4201      DATA  cnt=2               0     1    30   00000100
01AC [ 8] 460A      DSC2  cnt=11              0     1    30   00000108
01AE [ 9] 40C3      CODE  cnt=196             0     1    30   00000160
01B0 [10] 8007      DELT  delta=8
01B2 [11] 4008      CODE  cnt=9               0     1    30   00000478
01B4 [12] 804B      DELT  delta=76
01B6 [13] 400F      CODE  cnt=16              0     1    30   000004E8
01B8 [14] A000 195C LABS  offset=0x195C
01BC [16] 4020      CODE  cnt=33              0     1    30   0000195C

     ------ Loader Export Symbol Table ------
         Section    Address       Class     [Hashword]    Export Name
0478 [0]    1       000018DC     Data       [0014BDE0]    TheDriverDescription
0482 [1]    1       00000150     TVector    [000DE8E1]    CFMInitialize
048C [2]    1       00000148     TVector    [000AD1FD]    DoDriverIO
0496 [3]    1       00000140     TVector    [000CE94D]    CFMTerminate
04A0 [4]    1       00000118     TVector    [00071A43]    LoadSIM

04AA There are 6 (pad?) bytes at the end of this section.

DumpPEF complete - no errors reported.

